SURFACE MOUNT SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 두 개의 8” 유닛이 장착된 서브우퍼 기기이다. 8” 우퍼에는 다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있어야 하고 36Hz 이하의 우수한 저역 재생을 위한 대구경 포트가 있어야 한다. 120Hz 로우 패스 필터를 내장하고 외장 크로스오버 기기를 사용할 경우에는 전면 배플에서 필터를 통과시킬 수 있어야 하며 하이임피던스용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Surface mount bandpass subwoofer,

ported

- Low-frequency transducer	: Dual 8”(200mm) weather resistant,	polypropylene cone woofers,

rubber surround

- Frequency range

Frequency response(-6dB)	: 42Hz~165Hz

Useable frequency range(-10dB)	: 36Hz~205Hz

- Filter	: 120Hz low-pass, passive,

bypassable

- Maximum output

Calculated peak/continuous output

2π(half space)	: 124dB SPL/118dB SPL

4π(full space)	: 118dB SPL/112dB SPL

- Nominal impedance	: 8Ω

- Power rating

RMS power handling	: 250W(2hours IEC)

Recommended max amp power	: 500W RMS

- Sensitivity	: 94dB, 2.83V, 1m, half space(2π)

- Transformers

Type	: Custom low distortion laminated

core, wide bandwidth design

Taps	: 70V: 200, 100, 50, 25 W/

100V: 200, 100, 15 W/

8Ω selected by switch

Environmental	: Exceeds mil spec 810 for humidity,

salt spray and dust; IEC 60529

IP-X4 splash rating

[Enclosure details]

- Material	: Marine grade plywood, ABS,

steel grille

- Finish	: Textured black paint

- Grille	: Painted steel

- Connectors	: 4position barrier strip; 2in/2out

- Weight(net/shipping)	: 43lb(19.5kg)/55lb(25kg)

** AD-S28Tw 또는 동등 이상품 이어야 한다.