SURFACE MOUNT SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 서브우퍼 스피커로 DMT(Directivity Matched Transition) 기능으로 음의 영역을 균일하게하고 부드러운 주파수 응답을 보장하여야 한다. IEC60529 IP-54 등급으로 먼지와 얼룩 저항성 및 방수가 가능하여야 한다. 내후성을 강화하기위해 밀폐형 입력패널 덥개와 분말 코팅된 알루미늄 그릴을 사용하여야 한다. 내장된 스피커 브라켓은 특허받은 X-MOUNT 기술로 스피커를 쉽고 빠르게 설치하며 설치후 변형이 없어야 한다. 로우 임피던스와 하이임피던스를 선택하여 사용이 가능하도록 하여 다양한 앰프와 연동하여 사용이 가능하여야 한다. 이 통합된 기기이어야 한다.

(2) 기기특성

[System details]

Effective frequency range	: 30~135Hz

- Rated noise power/voltage	: 300watts/50volts(rms)

- Broad-band sensitivity	: 90dB SPL

- Maximum continuous SPL	: 115dB

- Maximum peak SPL	: 121dB

- Rated impedance	: 8ohms

- Recommended amplifier	: 600watts

- LF transducer	: 12” weather resistant paper cone

woofer, 2.5”/64mm voice coil

- Input connector type	: Euroblock connector with

parallel output

[Enclosure details]

- Enclosure material	: Painted ABS polymer

Grille material	: Powder coated aluminum

- Yoke material	: Powder coated galvanized steel

- Ingress protection	: IP-54

- Operating environment	: Designed for indoor and

outdoor use

- Testing	: The AD series loudspeakers

qualified for outdoor use using

the following tests:

Salt fog: MIL-STD-810G Method

509.5 for 100hours.

Humidity: MIL-STD-810G Method

507.5, natural cycle B2, cyclic high

RH for 7days

High and low temperature: tested

to QSC internal standards between

-20° and 50°C

- Operating temperature	: -20 to 50°C/-4 to 122°F

Weight

Net	: 29Ib(13.2kg)

Shipping	: 43.1Ib(19.6kg)

- Product dimensions	: 23.4” x 13.9” x 12.7”

(594 x 354 x 323mm)

Shipping dimensions	: 27.5” x 21.75” x 18.5”

(698 x 552 x 470mm)

** AD-S112sw 또는 동등 이상품 이어야 한다.