SURFACE MOUNT LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 2Way 스피커로 DMT(Directivity Matched Transition) 기능으로 음의 영역을 균일하게하고 부드러운 주파수 응답을 보장하여야 한다. IEC60529 IP-54 등급으로 먼지와 얼룩 저항성 및 방수가 가능하여야 한다. 내후성을 강화하기위해 밀폐형 입력패널 덥개와 분말 코팅된 알루미늄 그릴을 사용하여야 한다. 내장된 스피커 브라켓은 특허받은 X-MOUNT 기술로 스피커를 쉽고 빠르게 설치하며 설치후 변형이 없어야 한다. 로우 임피던스와 하이임피던스를 선택하여 사용이 가능하도록 하여 다양한 앰프와 연동하여 사용이 가능하여야 한다. 이 통합된 기기이어야 한다.

(2) 기기특성

[System details]

Effective frequency range	: 52Hz~20kHz

Rated noise power/voltage	: 300watts/50volts(rms)

Broad-band Sensitivity	: 95dB SPL

Directivity factor(Q)	: 12

Directivity index	: 11dB

Maximum continuous SPL	: 120dB

Maximum peak SPL	: 126dB

Rated impedance	: 8ohms

Recommended amplifier power	: 600watts

HF transducer	: 1” exit/1.4” voice-coil compression

driver

LF transducer	: 12” weather resistant paper cone

woofer, 2.5”/64mm voice-coil

Input connector type	: Euroblock connector with

parallel output

[Enclosure details]

Enclosure material	: Painted ABS polymer

Grille materia	: Powder coated aluminum

X-Mount material	: Powder coated aluminum

Ingress protection	: IP-54

Operating environment	: Designed for indoor and

: outdoor use

Testing	: The AD Series loudspeakers

qualified for outdoor

use using the following tests:

Salt fog: MIL-STD-810G method

509.5 for 100hrs.

Humidity: MIL-STD-810G method

507.5, natural cycle B2, cyclic high

RH for 7days

High and low temperature:

tested to QSC internal

standards between -20° and 50°C

Operating temperature range	: -20 to 50°C(-4 to 122°F)

Weight

Net	: 35.2Ib(16kg)

Shipping	: 46.3Ib(21kg)

Product dimensions(diameter x height)	: 23.4” x 13.9” x 12.7”

(594 x 354 x 323mm)

Shipping dimensions(HxWxD)	: 34.5” x 17.9” x 17.2”

(765mm, 455mm, 437mm)

** AD-S12 또는 동등 이상품 이어야 한다.