LOUD SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 10인치 2Way 스피커로 DMT(Directivity Matched Transition) 기능으로 음의 영역을 균일하게 하고 부드러운 주파수 응답을 보장하여야 한다. IEC60529 IP-54 등급으로 먼지와 얼룩 저항성 및 방수가 가능하여야 한다. 내후성을 강화하기 위해 밀폐형 입력패널 덥개와 분말 코팅된 알루미늄 그릴을 사용하여야 한다. 내장된 스피커 브라켓은 특허받은 X-MOUNT 기술로 스피커를 쉽고 빠르게 설치하며 설치후 변형이 없어야 한다. 로우 임피던스와 하이 임피던스를 선택하여 사용이 가능하도록 하여 다양한 앰프와 연동하여 사용이 가능하여야 한다. 이 통합된 기기이어야 한다.

(2) 기기특성

- Effective frequency range	: 50Hz~19kHz

- Rated noise power/voltage	: 250watts/45volts (rms)

- Broad-band sensitivity	: 92dB SPL

- Coverage angle(-6dB)	: 90°

- Directivity factor(Q)	: 10

- Directivity index	: 10dB

- Maximum continuous SPL	: 116dB

- Maximum peak SPL	: 122dB

- Rated impedance	: 8ohms

- Recommended amplifier power	: 500watts

- Transformer taps

70V	: 100, 50, 25, 12.5 watts and
8ohm bypass

100V	: 100, 50, 25 watts and
8ohm bypass

- HF transducer	: 1” exit/1.4” voice-coil compression
driver

- LF transducer	: 10” weather resistant paper cone
woofer, 2.5”/64 mm voice-coil

- Input connector type	: Euroblock connector with parallel
output

- Enclosure material	: Painted ABS polymer

- Grille material	: Powder coated aluminum

- X-Mount material	: Powder coated aluminum

- Enclosure details

Ingress protection	: IP-54

Operating environment	: Designed for indoor and outdoor
use

Testing	: The AD Series loudspeakers
qualified for outdoor use using the
following tests;
Salt fog; MIL-STD-810G Method
509.5 for 100 hrs.
Humidity; MIL-STD-810G Method
507.5, Natural cycle B2, cyclic high
RH for 7 days
High and low temperature; tested
to QSC internal standards between
-20° and 50° C

Operating temperature range	: -20 to 50 °C/-4 to 122 °F

- Net weight	: 31lb/15kg

- Product dimensions	: 20.3” x 12.5” x 11.7”
(516 x 318 x 298 mm)

- Shipping weight	: 40.6lb/18.45kg

- Shipping dimensions	: 31.7” x 16.1” X 16.1”
(805 x 409 x 409 mm)

** AD-S10T 또는 동등 이상품 이어야 한다.