LOUD SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 2Way 스피커로 DMT(Directivity Matched Transition) 기능으로 음의 영역을 균일하게 하고 부드러운 주파수 응답을 보장하여야 한다. IEC60529 IP-54 등급으로 먼지와 얼룩 저항성 및 방수가 가능하여야 한다. 내후성을 강화하기 위해 밀폐형 입력패널 덥개와 분말 코팅된 알루미늄 그릴을 사용하여야 한다. 내장된 스피커 브라켓은 특허받은 X-MOUNT 기술로 스피커를 쉽고 빠르게 설치하며 설치후 변형이 없어야 한다. 로우 임피던스와 하이 임피던스를 선택하여 사용이 가능하도록 하여 다양한 앰프와 연동하여 사용이 가능하여야 한다. 이 통합된 기기이어야 한다.

(2) 기기특성

- Effective frequency range	: 55Hz~20kHz

- Rated noise power/voltage	: 200watts/40volts (rms)

- Broad-band sensitivity	: 90dB SPL

- Coverage angle(-6dB)	: 105°

- Directivity factor(Q)	: 7

- Directivity index	: 9dB

- Maximum continuous SPL	: 113dB

- Maximum peak SPL	: 119dB

- Rated impedance	: 8ohms

- Recommended amplifier power	: 400watts

- Transformer taps

70V	: 60, 30, 15, 7.5 watts and
8ohm bypass

100V	: 60, 30, 15 watts and
8ohm bypass

- HF transducer	: 1” exit/1.4” voice-coil compression
driver

- LF transducer	: 8” weather resistant paper cone
woofer, 2.5”/51 mm voice-coil

- Input connector type	: Euroblock connector with parallel
output

- Enclosure material	: Painted ABS polymer

- Grille material	: Powder coated aluminum

- X-Mount material	: Powder coated aluminum

- Enclosure details

Ingress protection	: IP-54

Operating environment	: Designed for indoor and outdoor
use

Testing	: The AD Series loudspeakers
qualified for outdoor use using the
following tests;
Salt fog; MIL-STD-810G Method
509.5 for 100 hrs.
Humidity; MIL-STD-810G Method
507.5, Natural cycle B2, cyclic high
RH for 7 days
High and low temperature; tested
to QSC internal standards between
-20° and 50° C

Operating temperature range	: -20 to 50 °C/-4 to 122 °F

- Net weight	: 24.1lb/11kg

- Product dimensions	: 17.3” x 10” x 9.9”
(440 x 254 x 251 mm)

- Shipping weight	: 32.1lb/14.5kg

- Shipping dimensions	: 24.3” x 13.8” X 13.8”
(729 x 351 x 351 mm)

** AD-S8T 또는 동등 이상품 이어야 한다.