LOUD SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 4.5인치 2Way 천장형 스피커로 4인치 우퍼에는 다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있고 밀폐형 인클로저는 70Hz 이하의 저주파를 전달하는 데에 최적화되어 있어야 하며 우퍼와 선대칭으로 장착된 기존의 트위터 타입에서 자주 발생하던 간섭 현상을 줄이기 위해, 트위터는 우퍼의 중심부에서 약간 빗겨 장착이 되어 있어야 한다. 하이임피던스 용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

- HF transducer	: 19mm[.75in] silk dome tweeter
19mm[.75in] voice-coil horn loaded

- LF transducer	: 100mm[4.5in] weather treated
paper cone woofer,
25mm[1in] voice-coil

- Effective frequency range	: 68Hz~20kHz

- Rated noise power/voltage	: 50watts/20volts (rms)

- Broad-band sensitivity	: 87dB SPL

- Coverage angle(-6dB)	: 120°

- Directivity factor(Q)	: 6

- Directivity index	: 8dB

- Maximum continuous SPL	: 104dB

- Maximum peak SPL	: 110dB

- Rated impedance	: 8ohms

- Recommended amplifier power	: 100watts

- Transformer taps

70V	: 30, 15, 7.5, 3.75 watts and
8ohm bypass

100V	: 30, 15, 7.5 watts and
8ohm bypass

- Input connector type	: Euroblock connector with parallel
output

- Enclosure material	: Painted ABS polymer

- Grille material	: Powder coated aluminum

- X-mount material	: Powder coated aluminum

- Enclosure details

Ingress protection	: IP-54

Operating environment	: Designed for indoor and outdoor
use

Testing	: The AD Series loudspeakers
qualified for outdoor use using the
following tests;
Salt fog; MIL-STD-810G Method
509.5 for 100 hrs.
Humidity; MIL-STD-810G Method
507.5, Natural cycle B2, cyclic high
RH for 7 days
High and low temperature; tested
to QSC internal standards between
-20° and 50° C

Operating temperature range	: -20 to 50 °C [-4 to 122 °F]

- Net weight	: 2.9kg[6.5lb]

- Product dimensions	: 261 x 161 x 163 mm
[10.27 x 6.34 x 6.42 in]

- Shipping weight	: 7.65kg[16.8lb](pair packed)

- Shipping dimensions	: 394 x 261 x 458 mm
[15.5 x 10.3 x 18 in]
(pair packed)

** AD-S4T 또는 동등 이상품 이어야 한다.