SURFACE MOUNT SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 2Way 스피커로 파우더 코팅 알루미늄 그릴로 제작되어 가벼운 다용도 본체로 내구성이 뛰어나고 방습/방한성 (Weather Resistant)의 인클로저로 구성되어 있어야 한다. HF드라이버에는 Advanced Directivity ™ Rotatable Waveguide 순환식 도파관으로 본체 설치 방향과 관계없이 원하는 방향으로 스피커에서 정확한 사운드 전달이 가능하고 신호의 과 입력으로부터 스피커를 보호해주는 Dynamic Power Protection을 통해 최적의 파워핸들링이 가능한 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Compact 2-way, ported enclosure

Transducers

Low-frequency tranducers	: Dual 8” high power, treated paper

cone, 2” voice coil, neodymium

magnet

High-frequency tranducer	: 1” high output compression driver

- Frequency range

Frequency response(-6dB)	: 80Hz~27.7kHz

Useable frequency range(-10dB)	: 60Hz~29.5kHz

- Maximum output

Fullrange(passive mode)(continuous/max)	: 120/126W

LF(biamp mode)(continuous/max)	: 124/130W

HF(biamp mode)(continuous/max)	: 121/127W

- Nominal impedance

Passive	: 8Ω

LF	: 8Ω

HF	: 8Ω

- Power rating

Passive	: 450W(IEC 8hours)

LF	: 500W(IEC 8hours, 50Hz~2kHz)

HF	: 45W(IEC 8hours, 2kHz~20kHz)

- Recommended max amp power

Passive	: 900W RMS

- Sensitivity

Passive	: 93dB(100Hz~10kHz)

LF	: 97dB(200Hz~2kHz)

HF	: 104dB(2kHz~10kHz)

Nominal coverage	: 90°H x 60°V(-6 dB)

rotatable to 60°H x 90°V

Bass loading	: Ported, tuned to 60Hz

- Transformers

Type	: Custom low distortion laminated

core, wide bandwidth design

Taps	: 70V: 200, 100, 50, 25Watts/

100V: 200, 100, 50Watts/

8Ω bypass on AD-S282HT

[Enclosure details]

- Material	: Injection molded, weather resistant

high impact polystyrene

- Finish	: White or black(paintable)

- Weather resistance	: yes

- Grille	: Heavy duty powder coated

aluminum

- Connectors	: Barrier strip(switchable:

passive/active on AD-S282H)

- Weight(net/shipping)	: 27.7lb(12.6kg)/35.6lb(16.1kg)

** AD-S282H 또는 동등 이상품 이어야 한다.