PENDANT MOUNT LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 펜던트 스피커로 일정한 출력의 평탄한 음을 재생 가능하게 하는 DMT™기능이 있어야 하며, 하이임피던스용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V지원할 수 있어야 한다.

(2) 기기특성

[System details]

LF transducer	: 165mm(6.5”) weather treated

paper cone woofer

HF transducer	: 19mm(0.75”) aluminum dome

tweeter

Effective frequency range	: 56Hz~20kHz

Rated noise power/voltage	: 60watts/31volts(rms)

Sensitivity(dB)	: 88

Sensitivity at 4m, 100V maximum tap	: TBD

Rated coverage(‐6dB)	: 135° conical DMT™

Directivity factor	: 6.5

Directivity index(dB)	: 8

Maximum continuous SPL(dB)	: 106

Maximum peak SPL(dB)	: 112

Nominal impedance(ohms)	: 16

Recommended amplifier	: 120watts

Transformer taps/impedance	: 16Ω(in bypass setting)

7.5W(70V); 15W(100V) tap:667Ω

15W(70V); 30W(100V) tap:333Ω

30W(70V); 60W(100V) tap:167Ω

60W(70V); N/A(100V) tap:83Ω

Input connector type	: Euroblock connector with

parallel output

[Enclosure details]

Enclosure material	: Flame retardant ABS 765A VO

baffle and back can

Grille material	: Powder coated steel

Ingress protection	: IP-34

Operating environment	: Designed for indoor use

Operating temperature range	: -20 to 50°C(-4 to 122°F)

Weight

Net	: 4.1kg(9Ib)

Shipping	: 5.4kg(11.8Ib)

Product dimensions(diameter x height)	: Ø287 x 323mm(Ø11.3 x 12.7in)

Shipping dimensions(HxWxD)	: 343 x 406 x 356mm

(13.5 x 16 x 14in)

** AD-P6T 또는 동등 이상품 이어야 한다.