INSTALLATION LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2-웨이 패시브 라우드스피커로 90° 선대칭 방사 패턴의 12인치 우퍼와 3인치 코일 컴프레션 드라이버로 구성되어 있어야 한다. 컴프레션 드라이버가 크로스오버 부근에서 우퍼의 지향각과 자연스럽게 일치하도록 디자인한 DMT™ (Directivity Matched Transition) 기술의 결과로 균일한 출력을 재생하여야 한다. 앰프의 채널 수를 최소화하기 위해 패시브(풀레인지) 모드로 사용할 수도 있고 최상의 컨트롤과 성능을 제공하기 위해 바이앰프 모드로 사용할 수 있어야 한다.

(2) 기기특성

[System details]

Frequency range(-10dB)	: 48Hz~18kHz

Power capacity	: 550W/60V continuous

System sensitivity	: 95dB, 1W@1m

Coverage angle	: 90˚axisymmetric

Directivity factor(Q)	: 6.0

Directivity index(DI)	: 7.8

Recommended crossover	: 950Hz, 48dB/octave

- Maximum rated SPL

Passive	: 122dB @1m, continuous

128dB @1m, peak

- Rated impedance	: 8Ω

- HF transducer	: 76mm(3-inch) voice-coil,

compression driver; 72W/24V(2hrs)

- LF transducer	: 305mm(12in) driver with

102mm(4in) VC; 550W/60V(2hrs)

- Input connector	: Covered barrier strip, NL4

connector

[Enclosure details]

- Enclosure material	: 15-ply baltic birch plywood

Attachment points	: 15x M10 threaded inserts

Color	: Black(RAL 9011), White(RAL 9010)

Grille	: 16 gauge powder coated steel

Dimensions(HxWxD)	: 660mm x 381mm x 330mm

(26” x 15” x 13”)

Weight

Net	: 29.5kg(65Ib)

Shipping	: 32.6kg(72Ib)

- Shipping carton dimensions(HxWxD)	: 705mm x 484mm x 435mm

(27.8 x 19 x 17-inches)

** AP-5122 또는 동등 이상품 이어야 한다.