INSTALLATION LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2-웨이 패시브 스피커로 90° 선대칭 방사 패턴의 12인치 우퍼와 1.75인치 코일 컴프레션 드라이버로 구성되어 있어야 한다. 컴프레션 드라이버가 크로스오버 부근에서 우퍼의 지향각과 자연스럽게 일치하도록 디자인한 DMT™ (Directivity Matched Transition) 기술의 결과로 균일한 출력을 재생하여야 한다. 앰프의 채널 수를 최소화하기 위해 패시브(풀레인지) 모드로 사용할 수도 있고 최상의 컨트롤과 성능을 제공하기 위해 바이앰프 모드로 사용할 수 있어야 한다. 또한, 플로어 모니터용이나 라우드 스피커 스탠드에 폴 마운트 배치용으로 사용할 수 있어야 한다.

(2) 기기특성

[System details]

Effective frequency range	: 55Hz~20kHz

- Rated noise power/voltage	: 325W/36V continuous

System sensitivity	: 96dB, 1W@1m

Coverage angle	: 90˚conical DMT

Directivity factor(Q)	: 6.3

Directivity index(DI)	: 8.0

- Maximum rated SPL	: 121dB @1m, continuous

127dB @1m, peak

- Rated impedance	: 4Ω

- HF transducer	: 25mm(1in) compression driver

45mm(1.75in) voice-coil

- LF transducer	: 305mm(12in) weather resistant

cone woofer

64mm(2.5in) voice-coil

- Input connector	: 2 x NL4 in parallel, 2+/- thru

[Enclosure details]

- Enclosure material	: 15mm baltic birch plywood

Attachment points	: 11x M10 threaded inserts

Color	: Black(RAL 9011)

Grille	: 1.65mm(16 gauge) powder coated

steel

Dimensions(HxWxD)	: 510 x 385 x 370mm

(20.1 x 15.1 x 14.5in)

Weight

Net	: 18.1Ib(39.7kg)

Shipping	: 21.3Ib(46.7kg)

- Shipping carton dimensions(HxWxD)	: 570 x 505 x 495mm

(22.5 x 19.8 x 19.4in)

** AP-4122m 또는 동등 이상품 이어야 한다.