SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 18인치 800W 서브우퍼 스피커로 알루미늄 프레임 고성능 우퍼이며, 댄스 음악 킥 드럼과 베이스 라이브 공연에 적합해야 하고 37Hz까지 저역주파수 재생이 가능하여야 한다.

(2) 기기특성

- Configuration	: 1 x 18-inch, subwoofer,
non-powered

- Frequency response(-6dB)	: 37Hz to 230Hz

- Frequency range(-10dB)	: 32Hz to 230Hz

- Power capacity; continuous/peak	: 800W/3,200W

- Sensitivity	: 98dB, 1W @1m

- Coverage angle	: N/A

- Output(peak SPL @1m)	: 133dB

LF	: 457mm(18-inch) driver
with 102mm(4-inch) voice coil

HF	: N/A

- Nominal impedance	: 4Ω

- Cross-over	: Recommended 80~120 Hz LPF

- Input connectors	: 2 x NL4, 1 x barrier strip

- Enclosure	: Rectangular, plywood, black texture
paint finish. Four side-mounted
handles.
Rear panels provision for optional
4-inch casters. Perforated,
powder-coated steel grille with
foam lining.

- Mounting and Suspension	: M20 threaded pole-mount socket
24in(610mm) pole included

- Dimensions(W x H x D)	: 23.2 x 24.2 x 23.8 in
590 x 616 x 605 mm

- Net weight	: 43kg/95lb

- Shipping weight	: 48kg/106lb

** E118sw 또는 동등 이상품 이어야 한다.