SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2-웨이 패시브 라우드 스피커로 85° 선대칭 방사 패턴의 12인치 우퍼와 1.75인치 코일 컴프레션 드라이버로 구성되어 있어야 한다. 컴프레션 드라이버가 크로스오버 부근에서 우퍼의 지향각과 자연스럽게 일치하도록 디자인한 DMT™(Directivity Matched Transition) 기술의 결과로 균일한 출력을 재생하여야 한다.

(2) 기기특성

- Configuration	: 1 x 12-inch, 2-way, non-powered

- Frequency response(-6dB)	: 64Hz~20kHz

- Frequency range(-10dB)	: 46Hz~20kHz

- Power capacity; continuous/peak	: 400W/1,600W

- Sensitivity	: 96dB, 1W @1m

- Coverage angle	: 85° conical DMT

- Output(peak SPL @1m)	: 128dB

LF	: 305mm(12-inch) driver
with 76mm(3-inch) voice coil

HF	: 25mm(1-inch) exit,

45mm(1.75-inch) voice coil,
compression driver

- Nominal impedance	: 8Ω

- Cross-over	: Full-range only, 1.8kHz

- Input connectors	: 2 x NL4 1 x barrier strip

- Enclosure	: Trapezoidal, plywood, black texture
paint finish. Two side mounted
handles. Perforated, powdercoated
steel grille with foam lining.

- Dimensions(W x H x D)	: 14.2 x 24.2 x 14.6 in
360 x 616 x 371 mm

- Net weight	: 23kg/51lb

- Shipping weight	: 26kg/57.5lb

** E112 또는 동등 이상품 이어야 한다.