SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2-웨이 패시브 라우드 스피커로 85° 선대칭 방사 패턴의 10인치 우퍼와 1.75인치 코일 컴프레션 드라이버로 구성되어 있어야 한다. 컴프레션 드라이버가 크로스오버 부근에서 우퍼의 지향각과 자연스럽게 일치하도록 디자인한 DMT™(Directivity Matched Transition) 기술의 결과로 균일한 출력을 재생하여야 한다.

(2) 기기특성

- Configuration	: 1 x 10-inch, 2-way, non-powered

- Frequency range(-10dB)	: 50Hz~20kHz

- Power capacity; continuous/peak	: 300W/1,200W

- Sensitivity	: 95dB, 1W @1m

- Coverage angle	: 85° conical DMT

- Output(peak SPL @1m)	: 126dB

LF	: 254mm(10-inch) driver
with 64mm(2.5-inch) voice coil

HF	: 25mm(1-inch) exit,
45mm(1.75-inch) voice coil,
compression driver

- Nominal impedance	: 8Ω

- Cross-over	: Full-range only, 1.8kHz

- Input connectors	: 2 x NL4 1 x barrier strip

- Enclosure	: Multi-angle, plywood, black texture
paint finish, one top mounted
handle, perforated, powder-coated
steel grille with foam lining

- Mounting and suspension	: 6 x M8 suspension points,
dual angle, 35mm pole-socket

- Dimensions(W x H x D)	: 14.2 x 24.2 x 14.6 in
360 x 616 x 371 mm

- Net weight	: 20kg/44lb

- Shipping weight	: 23kg/50lb

- Dimensions(W x H x D)	: 13 x 22 x 13 in
(330 x 560 x 330 mm)

** E110 또는 동등 이상품 이어야 한다.