POWERED SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 파워드 서브우퍼 스피커로서 최대 132dB의 음압 출력이 가능하고 39Hz까지 재생 가능하여야 하고 듀얼 12인치 저음 드라이버를 사용하여야 하며 인클로저는 6th order band pass 타입의 산업 표준 자작나무 합판으로 만들어져 있어야 하고 다른 라우드 스피커와 스피커 폴로 고정하여 사용 가능한 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Dual 6th-order bandpass cardioid

subwoofer

Transducers

Low-frequency	: 2 x 12-inch(305mm), cone

- Frequency response(6dB)	: 44Hz~104Hz

- Frequency range(-10dB)	: 39Hz~118kHz

Nominal coverage angle	: 180˚cardioid

(15dB rear rejection @ 70Hz)

Maximum rated SPL	: 132dB @ 1m(peak)

Amplifier	: Class D, 2 x 1,800W(peak)

Cooling	: Low-noise, variable speed fan

Controls	: Power on/off

Gain control

Rotary encoder

2 x selection buttons

Indicators	: 2 x power LED(front and rear)

Input signal LED

Limiter active LED

Connectors	: 2 x locking XLR/F 1/4” combo

2 x XLR/M(loop-thru output)

1 x locking IEC power connector

AC power input	: Universal power supply

100~240VAC, 50~60Hz

AC power consumption	: 100VAC, 3.6A/120VAC,

3.0A/240VAC, 1.7A

[Enclosure details]

Enclosure	: 18mm birch rlywood

Color	: Black(RAL9011)

Grille	: Internal woofer cover

Dimensions(HxWxD)	: 24.5 x 15.5 x 33.5inches

(622 x 394 x 851mm)

- Weight

Net	: 40.1kg(88.5Ibs)

Shipping	: 48.5kg(107Ibs)

** KS212C 또는 동등 이상품 이어야 한다.