ACTIVE LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 18인치 서브우퍼 스피커로 경량의 1000W 클래스 D 앰프를 내장한 스피커이어야 한다. DMT™ (Directivity Matched Transition)의 기술이 적용되어 모든 청음 영역에서 LF와 HF의 커버리지를 매칭 시켜 상쇄 되거나 지나치게 부스트 되는 주파수 영역을 제거할 수 있어야 하고 Intrinsic Correction™, DEEP™, GuardRail™ 등의 기술 등이 적용되어 평탄한 음압재생, 주파수 손상 없이 저음역 제어, 내장된 앰프를 클립핑 신호로 부터 보호할 수 있어야 하는 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: 18” subwoofer

Transducers

Low-frequency	: 18” cone transducer

Mid-frequency	: -

High-frequency	: -

Frequency response(-6dB)	: 40Hz~112kHz

frequency range(-10dB)	: 37Hz~129kHz

Nominal coverage(-6dB)	: -

- Maximum SPL	: 135dB peak

Amplifier

Power output	: 1000W class D continuous

input impedance(Ω)

Channel A XLR/1/4”

Mic gain setting	: 0dB, +12dB, +24dB +36dB

Balanced	: 38k, 10k, 2.66k, 660Ω

Unbalanced	: 19k, 5k, 1.33k, 330Ω

Channel B XLR/1/4”	: 38k balanced/19k unbalanced

Channel B RCA	: 10k

XLR/1/4”	: 38k ballanced/19k unbalanced

Controls	: Balanced female XLR/1/4”

line/mic level input,

balanced female XLR/1/4”

line level input,

dual balanced male,

XLR full range line level out,

balanced male XLR “mix” out,

stereo RCA line level input,

remote gain control,

locking IEC power connector

Cooling	: On demand, 50mm variable

speed fan

Amplifier projection	: Thermal limiting,

output overcurrent,

overtemperature muting,

guardrail™

- Transducer projection	: Thermal limiting, excursion limiting

AC power input	: Universal power supply

100~240VAC, 50~60Hz

AC power consumption 1/8th power	: 100VAC, 2.3A • 120VAC, 2.01A •

230VAC, 1.13A

[Enclosure details]

Enclosure	: 15mm painted birch plywood

Finish	: Black textured paint

Grille	: Black powder coated 16 gauge stee

Dimensions(HxWxD)	: 20.3”, 23.4”, 29.9”

(516mm x 595mm x 761mm)

- Weight(net)	: 93.6lb(42.5kg)

** KW181 또는 동등 이상품 이어야 한다.