ACTIVE LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 2Way 스피커로 경량의 2000W 클래스 D 앰프를 내장한 스피커이어야 한다. DMT™ (Directivity Matched Transition)의 기술이 적용되어 모든 청음 영역에서 LF와 HF의 커버리지를 매칭 시켜 상쇄 되거나 지나치게 부스트 되는 주파수 영역을 제거할 수 있어야 하고 Intrinsic Correction™, DEEP™, GuardRail™ 등의 기술 등이 적용되어 평탄한 음압재생, 주파수 손상 없이 저음역 제어, 내장된 앰프를 클립핑 신호로 부터 보호할 수 있어야 하는 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Multi-purpose, 2-way active

loudspeaker

- LF tranducers	: 305mm(12in) cone

- HF tranducer	: 35.6mm(1.4in) titanium diaphragm

compression driver

Frequency response(-6dB)	: 50Hz~20kHz

frequency range(-10dB)	: 45Hz~20kHz

Nominal coverage angle	: 75°axisymmetric

- Maximum rated SPL	: 132dB peak

Amplifier	: Class D

Peak: 1800W(LF), 225W(HF)

- Cooling	: Low-noise, variable speed fan

Controls	: Power

3 x level

Rotary encoder

2 x selection buttons

indicators	: Monochrome LCD display

45mm x 25.4mm(1.75in x 1in)

2 x power LED(front and rear)

3 x input signal LED

Input A mic selected LED

Input B HI-Z selected LED

Limiter active LED

Connectors	: 2 x locking XLR/F 1/4” combo

(mic/line input and Hi-Z/line input)

1 x 3.5mm TRS(stereo input)

2 x XLR/M(loop-thru output)

1 x XLR/M(mix output)

1 x locking IEC power connector

AC power input	: Universal power supply

100~240VAC, 50~60Hz

AC power consumption 1/8th power	: 100VAC, 2.1A • 120VAC, 1.9A •

240VAC, 1.1A

[Enclosure details]

Enclosure	: impact resistant ABS

Attachment points	: 2 x M10 threaded inserts plus

integrated Pull-Back

Color	: Black(RAL 9011)

- Grille	: 18 gauge powered coated steel,

internal cloth lining

Dimensions(HxWxD)	: 602 x 356 x 350mm

(23.7 x 14 x 13.8in)

- Weight

Net	: 17.7lb(39kg)

Shipping	: 21.7lb(47.8kg)

** K12.2 또는 동등 이상품 이어야 한다.