LINE ARRAY SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 듀얼 18인치 라인 어레이용 서브우퍼로서 10:1 design factor를 통해 8개 이상의 서브우퍼 지원이 가능하고 이동과 조작의 편리성을 위해 dolly가 부착되어 있으며 12개의 손잡이가 장착되어 있어야 한다. 4인치의 섬유유리 보이스 코일과 견고한 구조를 지니며 인클로저는 자작나무 재질로 독립적인 두 개의 내부 공간과 견고함을 위해 확장된 내부 버팀목을 통해 정확한 소리 재생이 가능한 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: 2 x 18” vented subwoofer

Transducers

Low-frequency	: 2 x 850W, 8Ω 18” woofer with a

4” voice coil, ceramic magnet

assembly

- Frequency response(±3dB)	: 37Hz~200Hz(without processing)

- Frequency range(-10dB)	: 37Hz~1kHz

- Nominal impedance	: 4Ω

Continuous power capacity/

recommended power	: 1,700W/3,000W

Sensitivity(1W at 1m)	: 101dB

- Maximum output(SPL at 1m)(continuous/peak)	: 133dB/139dB

[Enclosure details]

Cabinet type	: Vented, trapezoidal enclosure

Enclosure material	: Baltic birch plywood/36mm baffle

and side panels; 15 mm top and

bottom

- Grille	: 14 gauge powder coated steel

Connectors	: 2 x NL4 in parallel

Pin outs

Pins	: 1+/1- sub, 2+/2- NC

Attachcent points	: Integral, adjustable rigging system,

vertical splay adjustable in 1°

increments from 0°~10°

- Weight(net/shipping)	: 204lb(92.5kg)/244lb(110kg)

includes dolly

Dimensions(HxWxD)	: 21.3” x 45.9” x 34.75”

(541mm x 1166mm x 882mm)

** WL218-sw 또는 동등 이상품 이어야 한다.