LINE ARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이 스피커로서 바이 앰프 또는 트라이 앰프 모드로 사용이 가능하고 수직 배열 시스템으로서 2개의 10인치 우퍼가 장착되어 있고 한 드라이버가 저주파수를 커버하면 다른 드라이버의 범위는 중주파수 대에서 중/고역 크로스오버까지의 지점을 재생하여야 하고 고주파수 대역은 1.4인치 출구, 3인치 네오디뮴 압축 드라이버로 구성되며 광범위한 사용 범위 (수평 140˚)를 가능케 하는 다중 구경 회절 도파관에 설치되어 있어야 한다. 인클로저는 산업 표준 자작나무 합판으로 만들어져 있어야 하고 간단하고 유연하며 안전한 리깅(rigging)을 제공하는 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Bi-amp or tri-amp mode

Transducers

High-frequency	: 1.4” exit, 3” titanium diaphragm,

neodymium magnet assembly

Low-frequency	: 2 x 400 W, 16Ω 10” woofer,

3” voice coil, ceramic magnet

assembly

- Frequency response(±3dB)	: 55Hz~18kHz(with recommended

DSP processing)

- Frequency range(-10dB)	: 48Hz~20kHz(with recommended

DSP processing)

- Nominal impedance

HF	: 16Ω

LF bi-amp mode	: 8Ω

LF tri-amp mode	: 16Ω(x2)

Continuous power capacity/recommended power

HF	: 80W/300W(2hours, AES1984-

2method, 1~10kHz)

LF bi-amp mode	: 600W/1400W(2hours, AES1984-

2method, 80~800Hz)

LF tri-amp mode	: 400W/700W(x2)(2hours, AES1984-

2method, 80~800Hz)

Sensitivity(1W at 1m)

HF	: 107.5dB(single cabinet measured

in free space.)

LF	: 98dB(single cabinet measured in

free space. LF drivers connected in

parallel)

- Maximum output(SPL at 1m)(continuous/peak)

HF	: 127dB/133dB

LF	: 127dB/133dB

Nominal coverage

H	: 140°

V	: dependent on number of

elements used

[Enclosure details]

Cabinet type	: Ported / trapezoidal

Enclosure material	: altic birch plywood

- Grille	: Perforated, formed powder coated

steel

Connectors	: 2 x neutrik speakon NL8 in parallel

Pin outs(pins/bi-amp/tri-amp)	: 1+1-/LF/MF, 2+2-/NC/LF,

3+3-/NC/NC, 4+4-/HF/HF

Attachcent points	: tegral, adjustable rigging system,

vertical splay adjustable in 1°

increments from 0°~10°

- Weight(net/shipping)	: 83lb(37.7kg)/91lb(41.4kg)

Dimensions(HxWxD)	: 10.8” x 27.4” x 20.75”

(274mm x 696mm x 527mm)

** WL2102-w 또는 동등 이상품 이어야 한다.