LINE ARRAY SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이 서브우퍼 스피커로서 최대 135dB의 음압출력이 가능하고 32Hz까지 재생 가능하여야 하고 12인치 저음 드라이버와 4인치의 보이스 코일, 세라믹 자석을 사용하여야 하며 인클로저는 4th order band pass 타입의 산업 표준 자작나무 합판으로 만들어져 있어야 하고 간단하고 유연하며 안전한 리깅(rigging)을 제공하는 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Dual 12”, 4th order bandpass

subwoofer

Transducers

Low-frequency	: Dual, 12” woofer with a 4” voice

coil, ceramic magnet assembly

- Frequency response(±3dB)	: 40Hz~100kHz

- Frequency range(-10dB)	: 32Hz~107kHz

- Nominal impedance

HF	: -

MF	: -

LF	: 4Ω

Continuous power capacity

HF	: -

MF	: -

LF	: 1,100W

Sensitivity(1W at 1m)

HF	: -

MF	: -

LF	: 99dB SPL

- Maximum output(dB SPL at 1m)(continuous/peak)

HF	: -

MF	: -

LF	: 129dB/135dB

Nominal coverage

H	: -

V	: -

[Enclosure details]

Enclosure type	: 4th order bandpass

Enclosure material	: 15mm birch plywood

Finish	: Available in black(WL212-sw) or

white(WL212-sw-WH) paintable

- Grille	: -

Connectors	: 2 x NL8 in parallel

Pin outs	: 1+/1- sub; 2+/2- NC; 3+/3-

NC; 4+/4- NC

Attachcent points	: Integral, non-adjustable

- Weight(net/shipping)	: 109lb(49.4kg)/125lb(56.7kg)

Dimensions(HxWxD)	: 15” x 20” x 29”

(381mm x 508mm x 737mm)

** WL212-sw 또는 동등 이상품 이어야 한다.