LINE ARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이 스피커로서 트라이 앰프 사용이 가능하고 수직 배열 시스템으로서 2개의 8인치 우퍼가 장착되어 있고 한 드라이버가 저주파수를 커버하면 다른 드라이버의 범위는 중주파수 대에서 중/고역 크로스오버까지의 지점을 재생하여야 하고 고주파수 대역은 1.4인치 출구, 3인치 네오디뮴 압축 드라이버로 구성되며 광범위한 사용 범위 (수평 140˚)를 가능케 하는 다중 구경 회절 도파관에 설치되어 있어야 한다. 인클로저는 산업 표준 자작나무 합판으로 만들어져 있어야 하고 간단하고 유연하며 안전한 리깅(rigging)을 제공하는 기기이어야 한다.

(2) 기기특성

[System details]

- Configuration	: Dual 8”, 3-way, tri-amp line-array

Transducers

High-frequency	: 3” diaphragm, neodymium magnet

compression driver

Low-frequency	: Dual, 8” woofer, 2.5” voice coil

- Frequency response(±3dB)	: 68Hz~18kHz

- Frequency range(-10dB)	: 62Hz~20kHz

- Nominal impedance

HF	: 16Ω

MF	: 16Ω

LF	: 16Ω

Continuous power capacity

HF	: 85W

MF	: 250W

LF	: 250W

Sensitivity(1W at 1m)

HF	: 108dB SPL

MF	: 98dB SPL

LF	: 98dB SPL

- Maximum output(dB SPL at 1m)(continuous/peak)

HF	: 127dB/133dB

MF	: 122dB/128dB

LF	: 122dB/128dB

Nominal coverage

H	: 140°

V	: Dependent on number of

elements used

[Enclosure details]

Enclosure type	: Ported, trapezoida

Enclosure material	: 15mm birch plywood

Finish	: Available in black (WL3082) or

white (WL3082-WH) paintable

- Grille	: Perforated, 16awg steel, backed

with black/white cloth fabric

Connectors	: 2 x NL8 in parallel

Pin outs	: 1+/1- NC; 2+/2- LF; 3+/3-

MF; 4+/4- HF

Attachcent points	: Integral, side plate adjustable

rigging system, vertical splay

adjustable in 1° increments from

0°~10°

- Weight(net/shipping)	: 38lb(17kg)/45.5lb(20.7kg)

Dimensions(HxWxD)	: 9” x 20” x 16”

(229mm x 508mm x 406mm)

** WL3082 또는 동등 이상품 이어야 한다.