SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이 전용 서브우퍼 스피커로서 Bass-reflexs 엔클로저 구조의 단일 18인치 우퍼가 장착되어 있어야 한다. 850W의 정격 출력이 가능하고 29Hz까지 저역주파수 재생이 가능하여야 한다. WL2082-i와 최상단 또는 어레이 뒤에 설치가 가능하여야 하고 검정색 또는 흰색 선택이 가능한 기기이어야 한다.

(2) 기기특성

- Configuration	: Vented box

- Transducers

Low-frequency	: 850W, 8Ω 18" woofer with a 4“
voice coil, ceramic magnet
assembly

- Frequency response(±3dB)	: 32Hz~200Hz

- Frequency range(-10dB)	: 29Hz~800Hz

- Nominal impedance

LF	: 8Ω

- Continuous power capacity/Recommended power

LF	: 850W/1,750W

- Sensitivity(1W at 1m)

LF	: 98dB

- Maximum output continuous/peak (SPL at 1m)

LF	: 128.5dB/134.5dB

- Cabinet type	: Vented subwoofer

- Enclosure material	: 18mm baltic birch plywood

- Finish	: Available in black(WL118-sw BLK)
or white(WL118-sw WHT)
paintable

- Grille	: 16 gauge powder-coated steel with
cloth backing

- Connectors	: 2 x NL8 in parallel/
2 x NL4 in parallel

- Pin Outs

Pins(NL8)	Pins(NL4)

1+/1-	Sub	1+/1-	Sub

2+/2-	Pass thru	2+/2-	Pass thru

3+/3-	Pass thru

4+/4-	Pass thru

- Attachment points	: Integral, non-adjustable
(straight array only)

- Weight(Net/Shipping)	: 111lb(50.4kg)/121lb(55kg)

- Dimensions(HWD)	: 22.1" x 27.6" x 30.3“
(562mm x 702mm x 771mm)

** WL118-sw 또는 동등 이상품 이어야 한다.