LINE ARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이 스피커로서 바이 앰프 또는 트라이 앰프 모드로 사용이 가능하고 수직 배열 설치(Installation Line Array) 방법을 적용한 기기이어야 하며 2개의 8인치 우퍼가 장착되어 있고 1.75인치 네오디뮴 압축 드라이버 한 쌍이 광범위한 사용 범위(수평 140˚)를 가능케 하는 다중 구경 회절 도파관에 설치되어 있어야 한다. 검정색과 흰색의 두 가지 버전으로 어떠한 설치 환경에서도 잘 어울려야 하며 간단하고 유연하며 안전한 리깅(rigging)을 제공하는 기기이어야 한다.

(2) 기기특성

- Configuration	: 3-way, bi-amp or tri-amp mode

- Transducers

High-frequency	: Dual 50W, 8Ω 1" exit,
1.75" titanium diaphragm,
neodymium magnet assembly

Low-frequency	: Dual 200W, 16Ω 8" woofer,
2" voice coil, neodymium magnet
assembly, weather resistant cone

- Frequency response(±3dB)	: 80Hz~20kHz

- Frequency range(-10dB)	: 68Hz~22kHz

- Nominal impedance

HF	: 16Ω

LF bi-amp mode	: 8Ω

LF tri-amp mode	: 16Ω(x 2)

- Continuous power capacity/Recommended power

HF	: 100W/200W

LF bi-amp mode	: 400W/800W

LF tri-amp mode	: 200W/400W (x 2)

- Sensitivity(1W at 1m)

HF	: 106dB

LF	: 96dB

- Maximum output continuous/peak (SPL at 1m)

HF	: 126dB/132dB

LF	: 122dB/128dB

- Nominal coverage

H	: 140°

V	: dependent on number of elements
used

- Cabinet type	: Ported, elliptical/trapezoidal

- Enclosure material	: HIPS(high impact polystyrene) with
UV protectant

- Finish	: Available in black(WL2082-i BLK) or
white(WL2082-i WHT) paintable

- Grille	: Perforated, formed aluminum

- Connectors	: 2 x NL8 in parallel

- Pin Outs	: Pins	Bi-Amp	Tri-Amp

1+/1-	NC	NC

2+/2-	NC	LF2

3+/3-	LF	LF1

4+/4-	HF	HF

- Attachment points	: Integral, side plate adjustable
rigging system, vertical splay
adjustable in 1° increments from
0°~10°

- Weight(Net/Shipping)	: 37lb(16.8kg)/45lb(20.45kg)

- Dimensions(HWD)	: 11.8" x 27" x 13.4“
(300mm x 686mm x 340mm)

** WL2082i 또는 동등 이상품 이어야 한다.