POWERED SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 라인어레이용 18인치 서브우퍼로서 플라잉 및 스택 사용이 가능하게 설계되어 있으며 1,000W의 Class D 파워앰프를 내장한 기기로 DEEP™ DSP 알고리즘과 GuardRail™, Auto Standby의 기술이 적용되어 있으며 저역대 주파수의 지향성 컨트롤에 대한 스위치를 포함한 기기이어야 한다.

(2) 기기특성

- Configuration	: 18" ported subwoofer

- Transducers
Low-Frequency	: 18" cone transducer

- Frequency Response(-6dB)	: 38Hz

- Frequency Range(-10 dB)	: 33Hz

- Maximum SPL(1 meter)	: 135dB

- Amplifiers
Power Output	: 1,000W Class D continuous

- Input Impedance(Ω)	: XLR; 40k balanced/20k unbalanced

- Controls	: Power·Attenuation·LF Setting
(External Sub/Normal/DEEP™)·
Array Size(1-5)·Front LED(Pwr/
Limit/Off)

- Indicators	: Limit·Standby·Power·Signal

- Connectors	: Balanced female XLR line level
input·Balanced male XLR full range
line level out·Remote attenuation
control·Locking powerCON® power
connector AC out

- Cooling	: On demand, 50mm variable speed
fan

- Amplifier Protection	: Thermal limiting·Output
overcurrent·Overtemperature
muting·GuardRail™

- Transducer Protection	: Thermal limiting·Excursion limiting

- AC Power Input	: Universal power supply
100~240 VAC, 50~60 Hz

- AC Power Consumption	: 100VAC, 2.3A·120VAC, 2.01A·
230VAC, 1.13A

- Enclosure	: Painted birch plywood

Weight(Net)	: 104lbs(47.2kg)

Finish	: Black or White textured paint

Grille	: Black or White powder coated
16 gauge steel

- Dimensions(HWD)	: 21.6" x 23.4" x 25.7“
(547mm x 594mm x 653mm)

- Available Accessories	: KW181 Pole·KLA181 Cover·KLA181

M10 KIT·KLA AF12 Array Frame

** KLA181 또는 동등 이상품 이어야 한다.