NETWORK POWER AMPLIFIERS

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 디지털 프로세서를 내장한 8채널 LOW/HI 겸용 앰프로서, 크로스오버, 파라메트릭 EQ필터, 리미터 등의 기본 기능을 제공하여야 하며, 프로세서는 20가지 기본 설정이 내장되고 추가로 50가지의 프리셋이 저장, 사용상의 편의를 위해 사용하고자 하는 스피커의 기본 설정값이 내장되 프로그램으로 제공받아 간편하게 사용되며, GPIO 기능을 제공하여 외부기기로부터 접점을 제공하여 간편하게 ON/OFF 제어가 되는 기기이어야 한다.

또한 Q-LAN을 내장하고 있어 Q-SYS 프로세서 등과 연동되어 제어하거나, 네트워크로 입력 연결이 가능하여야 한다. 또한 Q-LAN을 내장하고 있어 Q-SYS 프로세서등과 연동되어 제어하거나, 네트워크로 입력 연결이 가능하여야 한다.

(2) 기기특성

- 8 independent channels

A, B, C, D, E, F, G, H

70V: 500W(Max power)/300W(Continuous power)

100V: 500W(Max power)/300W(Continuous power)

8Ω: 500W(Max power)/300W(Continuous power)

4Ω: 500W(Max power)/300W(Continuous power)

2Ω: 500W(Max power)/300W(Continuous power)

- 2 channels combined in BTL bridge
A+B or C+D or E+F or G+H
doubles voltage

8Ω: 1,000W(Max power)/600W(Continuous power)

4Ω: NR*/NR*

2Ω: NR*/NR*

- 2 channels combined in parallel
AB or CD or EF or GH
doubles current

8Ω: 1,000W(Max power)/600W(Continuous power)

4Ω: 1,000W(Max power)/600W(Continuous power)

2Ω: 1,000W(Max power)/600W(Continuous power)

- 3CH combined in parallel
ABC or EFG
triples current

8Ω: 1,000W(Max power)/900W(Continuous power)

4Ω: 1,500W(Max power)/900W(Continuous power)

2Ω: 1,500W(Max power)/900W(Continuous power)

- 4CH combined in bridged/parallel
AB+CD
doubles current and voltage

8Ω: 2,000W(Max power)/1,200W(Continuous power)

4Ω: 2,000W(Max power)/1,200W(Continuous power)

2Ω: NR*/NR*

- 4CH combined in parallel
ABCD or EFGH
quadruples current

8Ω: 1,200W(Max power)/1,200W(Continuous power)

4Ω: 2,000W(Max power)/1,200W(Continuous power)

2Ω: 2,000W(Max power)/1,200W(Continuous power)

- Typical distortion

8Ω	: 0.02~0.05%

4Ω	: 0.04~0.1%

- Maximum distortion

4Ω~8Ω	: 1.0%

- Frequency response(8Ω)	: 20Hz~20kHz+/-0.3dB

- Noise

Unweighted output unmuted	: >101dB

Weighted output muted	: >104dB

- Gain(1.2V setting)	: 38.4dB

- Damping factor	: >100

- Input impedance	: > 8k balanced and 4k unbalanced

- Input sensitivity

Continuously variable	: Vrms 1.23mV to 17.35V

dBu -56 to 27

dBv -58.2 to 24.8

- Controls and indicators(front)	: Power•channel mute buttons•

channel select buttons•

channel input

signal and clip LED indicators•

channel output and limit LED

meters•next, prev, ID buttons•

control knob

- Controls and indicators(rear)	: Euro(green) power disconnect

- Input connectors	: Q-LAN network connectivity only

- Output connectors	: 8-pin euro(green)

- Amplifier and load protection	: Short circuit, open circuit, thermal,

RF protection. on/off muting,

DC fault shutdown, active inrush

limiting

- AC power input	: Universal power supply

100~240 VAC, 50~60Hz

- Dimensions(HxWxD)	: 3.5” x 19” x 16”

(89mm x 482mm x 406mm)

- Weight(net/shipping)	: 25.0lb(11.3kg)/29lb(13.2kg)

** CXD8.4Qn 또는 동등 이상품 이어야 한다.