POWER AMPLIFIERS

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2채널 앰프로서 QSC PowerLight 기술을 특정 기능들과 결합하여 고정 설치 요건을 충족시켜야 하며 HD15 Data Port 커넥터가 있어 이를 QSControl(컴퓨터 제어 음향장치)와 연결하여 이더넷 망을 통해 앰프를 원격으로 모니터링, 제어를 할 수 있어야 한다. 최상의 음질과 고출력이 요구된 설치 환경에 적합한 기기이어야 하고, 다이렉트 70볼트 기능을 더해 분산 오디오 시스템에 적합하며 AC전원의 험 노이즈를 제거하고 음질을 개선시키면서도 앰프 자체 무게를 줄일 수 있는 PowerLight 전원 공급 기술을 채택한 기기이어야 한다.

(2) 기기특성

- Stereo mode(both channels driven)

8Ω/20Hz~20kHz/0.05% THD	: -

4Ω/20Hz~20kHz/0.05% THD	: -

2Ω/1kHZ/1% THD	: -

70V/20Hz~20 kHz/0.05% THD	: 200W

70V/1kHz/0.05% THD	: 250W

70V/1kHz/1% THD	: 300W

- Bridge mono mode

16Ω/20Hz~20kHz/0.1% THD	: -

8Ω/20Hz~20kHz/0.1% THD	: -

4Ω/1kHz/1% THD	: -

140V/20Hz~20kHz/0.1% THD	: 400W

140V/1kHz/0.05% THD	: 500W

140V/1kHz/1% THD	: 600W

- Signal to noise(20Hz~20kHz)	: > -106dB

- Input sensitivity at 8Ω	: 1.26Vrms

- Gain at 8Ω	: 35dB

- Output circuitry	: Class AB+B

- Distortion(SMPTE-IM)	: < 0.02%

- Distortion(typical)

20Hz~20kHz:10dB below rated power	: < 0.01% THD

1.0kHz and below: full rated power	: < 0.01% THD

- Frequency response	: 20Hz~20kHz, ±0.2dB

- Damping factor	: > 500

- Input impedance	: 6k ohms unbalanced,

12k ohms balanced

- Input clipping	: 10Vrms(+22dBu)

Cooling	: Variable speed fan,

rear-to-front air flow

- Connectors

Input	: 3-pin XLR&3-pin detachable

terminal blocks(1each per channel)

Output	: Safety shrouded barrier strip

- Amplifier protection	: Full short circuit, open circuit,

thermal, ultrasonic, RF protection.

stable into reactive or mismatched

loads

- Load protection	: On/off muting,

DC-fault power supply shutdown

- Dimensions(HxWxD)	: 3.5”(8.9cm) 2RU x 19”(48.3cm)

rack mounting x 14”(35.6cm)

from front mounting rails

- Weight

Net	: 21Ib(9.5kg)

Shipping	: 27Ib(12.3kg)

120V current consumption	: Idle/0.8A

1/8 power pink noise(typical of program	: 8Ω/-, 4Ω/-, 2Ω/-

material at maximum unclipped power)	70V/5.7A

1/3 power pink noise(typical of program	: 8Ω/-, 4Ω/-, 2Ω/-

material with servere clipping)	70V/8.0A

** CX302V 또는 동등 이상품 이어야 한다.