INTEGRATED DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Intel™ CPU 및 마더 보드뿐만 아니라 IMC가 개발한 전용 Linux™ 실시간 운영 체제를 활용하여 모든 규모의 AV시스템을 위한 동급 최고의 플래시 기능을 제공하여야 한다. 또한 Q-SYS 플랫폼에서 유연한 오디오 I/O를 제공하며, 아날로그, 디지털 및 네트워크 연결이 필요한 애플리케이션이 되어야 하며, 8개의 I/O카드 슬롯을 갖추고 있어 다양한 연결 옵션을 제공하여야 한다.

(2) 기기특성

- Description	: System processor and control
engine with integrated I/O
(or I/O expander when configured
via software as I/O-510i)

- Configuration modes	: “Q-SYS Core” - centralized
processor and control engine for
a Q-SYS system“I/O-510i
configuration suited to integrating
high channel-count networked
I/O cards (Dante, CobraNet, AVB)”
- peripheral to an additional
Q-SYS Core processor on the
system

- Supported peripherals(when configured as a Q-SYS Core Processor.)
: I/O-8 Flex Channel Expander,
I/O-USB Bridge, PTZ-IP Camera
series, I/O Frame, I/O-Frame 8s,
I/O-22, I/O-11 Series, Page Station
Series, TSC Series touch screens

- Software requirements	: Q-SYS Designer 6.x.x

[Channel Capacity]

- Network channel capacity	: 256 x 256 (in Q-SYS Core mode)/
128 x 128 (in I/O Frame mode)

- Local audio I/O capacity	: 8 audio I/O card slots
- accommodates up to 128 x 128
total onboard I/O channels

- AEC channel capacity	: 64 at 200ms tail length(available
when configured as a Q-SYS Core
Processor only)

- Multitrack player capacity	: 16 tracks, expandable to 128 tracks
(available when configured as
a Q-SYS Core Processor only)

- Media drive capacity	: Approximately 6GB on the default
drive(when configured as a Q-SYS
Core Processor only, upgrade
options are available)

- Configure to order inputs/outputs options

Audio I/O cards	: COL4; Line output card(4 channels)
CODP4; DataPort card(4 channels)
CIML4; Mic/line input card
(4 channels)
CIML4-HP; High Performance
mic/Line input card(4 channels)

CAES4; AES3 digital I/O card
(4x4 channels)
CIAES16; AES3 digital input card
(16 channels)
CCN32; CobraNet network bridge
card(up to 32 x 32 channels)

CAN32; AVB network bridge card
(up to 32 channels)

CDN64; Dante network bridge card
(up to 64x64 channels)

Media drives(in Q-SYS Core mode)	: M2-MD-S; 128GB
M2-MD-M; 256GB
M2-MD-L; 512GB

Multitrack players(MTP)(in Q-SYS Core mode)	: MTP-32; 32 tracks
MTP-64; 64 tracks

MTP-128; 128 tracks

[Controls and Indicators]

- Front panel controls	: “NEXT” OLED page forward
capacitive touch button
“ID” device identification capacitive
touch button
“Clear Network Settings” - invoked
when “NEXT” and “ID” are pressed
simultaneously

- Front panel connectors	: AUX USB; USB Host x2
(Type A connectors)

- Front panel indicators	: Blue “POWER” LED
304 x 96 monochrome OLED
display

- Rear panel connectors	: RS232; Male 9-pin D shell
connector(DE-9)

Video out; HDMI
AUX USB; USB Host x4
(Type A connectors)
AUX Network; RJ45
10/100/1000 Mbps

GPIO; Female 15-pin D shell
connector x2 (DA-15)

Media network LAN A; RJ45
1000Mbps(QLAN, AES67, VoIP,
WAN, Media Streaming, etc)

Media network LAN B; RJ45
1000Mbps(QLAN, AES67, VoIP,
WAN, Media Streaming, etc)
AC Mains Power; IEC connector

- Rear panel indicators	: “Link”, “Speed” and “Activity” LEDs
on all LAN ports

[Miscellaneous]

- Line voltage	: 100VAC~240VAC 50~60 Hz

- Current draw	: 3.7A Max @100VAC(actual current
draw depends on configuration
options such as I/O cards and/or
Media Drive, DSP loading and
network loading)

- Operating temperature range	: 0°C~50°C

- Storage temperature	: -20°C to +70°C

- BTU/Hour	: 600(power conversion estimate
under typical load)

- Humidty	: 5% to 85%

- Regulatory	: FCC 47 CFR Part 15 Class A,
IC ICES-003, CE (EN55032,
EN55035), EU RoHS directive
2011/65/EU, WEEE directive
2012/19/EU, China RoHS directive
GB/T26572, EAC, RCM, UL, C-UL,
EFUP 10, Expected Product Life
Cycle 20 years

- Product dimensions	: 3.5" x 19" x 15“
(89mm x 483mm x 381mm)

- Shipping carton dimensions	: 23.5" x 20" x 6.5“
(597mm x 508mm x 165mm)

- Shipping weight	: 23lbs. minimum(installation of I/O
cards increases shipping weight)

** Core 510i 또는 동등 이상품 이어야 한다.