DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 모든 오디오 라우팅과 프로세싱을 수행할 수 있어야 하고 모든 컨트롤 기능이 처리 가능하며 최대 각 512채널의 네트워크 오디오 입력과 출력을 수용할 수 있어야 한다. 중앙 처리 아키텍처를 기반으로 어떠한 입력이라도 복잡한 신호 경로를 거치지 않고 원하는 출력단으로 라우팅할 수 있으며 모든 처리가 한 기기에서 이루어져 설계자에게 완벽한 유연성을 제공하여야 한다.

Q-LAN 이라는 스탠다드 방식의 로우 레이턴시 기가비트 이더넷 네트워크로 실행되어야 하며 네트워크 3계층에 해당하는 기기이어야 하며, Q-LAN 포트를 지원하는 Q-SYS 장비끼리 연결되어 상호 통신이 가능한 기기여야 한다.

(2) 기기특성

[Hardware]

- Input frequency response

20Hz to 20kHz @+21dBu	: +0.05%/-0.5%

Platform	: Dell poweredge

R740(14th generation)

Chassis	: 2.5” hard drive

Power	: 2x hot-plug universal input 750W

PSU modules

LCD	: Single line scrolling display

LAN	: 4x 1000Mbps ports

(2x Q-SYS multimedia,

2x Q-SYS aux)

iDRAC8	: 1x dedicated 1000Mbps iDRAC v8,

enterprise license

Video	: 2x HD-15 VGA ports

(1x front panel, 1x rear panel)

USB	: 2x USB 2.0 host(front panel),

2x USB 3.0 host (rear panel)

Serial	: 1x DE-9 RS-232 port(rear panel),

16550-compliant

SATA SSD	: 960GB Q-SYS media drive

Additional info	: For additional hardware

specifications visit:

www.Dell.com/Dell/servers

[Controls and indicators]

Front panel	: Power button

ID button and indicator

(blinks when enabled from

Q-SYS designer software)

Rear panel	: ID button and indicator

(blinks when enabled from

Q-SYS designer software)

[Q-SYS capacities]

Network channels	: 512x512

AEC Processors	: 160

VoIP instances	: 64

Muti-trace player	: 16 included(upgradeable

to 32, 64 or 128 tracks)

[Packaging]

Shipping carton dimensions	: 940mm(37in.) x 610mm(24in.) x

280mm(11in.)

Weight(Shipping)	: 64lb(29kg)

** Core 5200 또는 동등 이상품 이어야 한다.