CHANNEL EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 입력소스 부근과 최종 목적지 부근에 위치하여 실제적으로 입출력을 연결하는데 사용하는 기기로서 듀얼 Gigabit Ethernet 연결을 통해 코어를 통해 처리되도록 오디오 신호를 전달해야 하며 중앙장치인 Main Core에 연결되어 중앙 집중 프로세싱 구조를 이루어야 한다. 최대 8채널의 입력 또는 출력이 제공 가능한 네트워크 3계층 기기이어야 한다. 또한 채널은 사용자가 원하는 입출력으로 유연하게 바꿀 수 있어야 한다.

(2) 기기특성

[Inputs/Outputs]

- Audio Flex Channel Capacity	: 8

- Audio Flex Channel Assignments	: Each channel can be configured as
a mic/line input or as a line output
(configured through Q-SYS
Designer software)

- Rear Panel Indicators	:  “Link”, “Speed” and “Activity”
LEDs on all LAN ports

[USB Inputs & Outputs]

- USB Audio Bridging	: Up to 8x8 channels of digital audio
in/out via software definable USB
instances advertised to the USB
Host operating system

- USB B (device port)
Bit depth	: 16-bit, 24-bit (configured in Q-SYS
Designer software)
USB Channel Capacity	: 8 x 8

Sample Rate	: 48kHz

[Controls]

- Front Panel Controls	: “NEXT” OLED page forward
capacitive touch button “ID” device
identification capacitive touch
button “Clear Network Settings”
- invoked when “NEXT” and “ID”
are pressed simultaneously

- Front Panel Connectors
AUX USB	: USB Host x2 (Type A onnectors)

- Rear Panel Connectors
Audio Flex I/O	: 12-pos blue Euro Block x2
GPIO	: 10-pos black Euro Block x2
(GPI = 1x10, GPO = 1x10)
RS232	: 3-pos black Euro Block
AUX USB Host	: USB Host x2 (Type A connectors)
AUX USB Device	: USB Device Port (Type B
connector)
Media Network LAN A/PoE+ Power In	: RJ45 1000 Mbps
Media Network LAN B	: RJ45 1000 Mbps
AUX PWR In	: 2-pos green Euro block

[GPIO]

- General Purpose Inputs	: 0-24VDC analog input or contact
closure

- General Purpose Outputs	: Open collector, 24VDC at 200mA
max, internal pullup to 3.3V

- GPIO 12 VDC Power Pins	: 12VDC out at 100mA max

- Product Dimensions	: 8.66" x 9.43" x 1.75“
(220mm x 240mm x 44mm),
1RU half rack

** I/O-8 Flex 또는 동등 이상품 이어야 한다.