I/O PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 입력소스 부근과 최종 목적지 부근에 위치하여 실제적으로 입출력을 연결하는데 사용하는 기기로서 듀얼 Gigabit Ethernet 연결을 통해 코어를 통해 처리되도록 오디오 신호를 전달해야하며 중앙장치인 MAIN CORE에 연결되어 중앙 집중 프로세싱 구조를 이루어야 한다. 4개의 입/출력 카드를 장착할 수 있어 최대 16채널의 입력 또는 출력이 제공 가능한 네트워크 3계층 기기이어야 한다.

(2) 기기특성

[System details]

System harware	: I/O Frame

Description	: System audio input and output

device

Front panel controls	: LCD page forward momentary

switch

Unit ID button momentary switch

Clear settings momentary switch

Front panel card receptacle	: -

Front panel indicators

Power on	: Blue LED

Device status	: Tri-color LED

Audio signal	: Five tri-color LEDs/per I/O card slot

240 x 64 monochrome LCD

graphics display

Rear panel connectors

RS-232	: DE-9(male 9-pin D shell connector)

GPIO	A	: DA-15

(female 15-pin D shell connector)

Q-SYS network LAN A	: RJ45 1000MBps only

Q-SYS network LAN B	: RJ45 1000MBps only

I/O Capacity	: Up to 16 x 16. requires purchase

of I/O cards

Line voltage requirements	: 100VAC~240VAC, 50~60Hz

Current draw	: 625mA(120V mains)

Thermal	: 205BTU/h(typical)

Dimensions(HWD)	: 1.75” x 19” x 15”

(44.45mm x 482.6mm x 381mm)

** I/O Frame 또는 동등 이상품 이어야 한다.