I/O PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 개별적으로 분산되어 있는 오디오 시스템을 설계할 때 적합한 소형 독립 장치로서, 2개의 마이크/라인 입력과 2개의 라인 출력을 제공하고, RS-232, 8개의 GPIO, USB, 원격 디스플레이 포트를 지원하며, PoE나 24 VDC를 통해서 선택적으로 전원 공급가능하다. 로컬모니터스피커 구동을 위해 8.5Watt 모노앰프가 포함되어 있는 기기이어야 한다. 또한 기가비트 이더넷을 직원하는 네트워크 Q-LAN 포트(RJ-45 이더넷 컨넥터)로 Q-SYS 장비끼리 상호 통신이 가능하여야 한다.

(2) 기기특성

[System details]

System harware	: I/O-22

Description	: System audio input and

output device

Panel controls	: Unit ID button momentary switch

Power indicators

Power on	: Green LED

Device status	: Tri-color LED

Locate/ID	: Green LED

Panel connectors

Mic/line	: 2 x 3-pin euro style connectors,

orange

Line out	: 2 x 3-pin euro style connectors,

green

GPIO	: 2 x 6-pin(8 signals, 4 ground)

euro style connectors

RS-232	: DE-9(male 9-pin D shell connector)

USB	: For future development

Remote display	: For future development

Speaker	: 2-pin female euro style connectors

Aux power	: 2-pin euro style connector

Q-SYS network LAN A	: RJ45 1000MBps only

Q-SYS network LAN B	: RJ45 1000MBps only

Input dynamic range	: Unweighted > 88dB

A-weighted > 91dB

Input frequency response(20Hz~20kHz)	: +/- 0.8dB

Input Impedance	: 10K ohms

Max input level

+12dBu gain setting	: 30.8mV

-8dBu gain setting	: 1.9V

-28dBu gain setting	: 3.09V

Distortion(20Hz~20kHz) at max input levels

+12dBu gain setting	: -70dB or 0.032%

-8dBu gain setting	: -57 or 0.14%

-28dBu gain setting	: -57 or 0.14%

Input crosstalk(20Hz~20kHz typical)	: -78dB(ch1 to ch2)

Common mode rejection(20Hz~20kHz)	: -39dB

Output dynamic range	: Unweighted > 104dB

A-weighted > 107dB

Output frequency response(20Hz~20kHz)	: +0.3dB to –0.5dB(line out)

Max output level	: +10dBu

Max speaker output power	: 9W into 4ohms

Output crosstalk(20Hz~20kHz typical)	: -74dB(ch1 to ch2)

Line voltage requirements	: IEEE 802.3af power over ethernet

(PoE) or +24V DC @ 1.5A min

Dimensions	: 1.75” x 8.875” x 5.875”

(44.45mm x 226.5mm x 149mm)

** I/O-22 또는 동등 이상품 이어야 한다.