TOUCH SCREEN CONTROLLER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 터치스크린 컨트롤러로 800 x 480 해상도, 밝기 400nit의 풀컬러 LCD를 사용해야 하며 Q-Sys 시스템을 간단한 세팅 변경에서부터 전체 스냅샷 리콜까지 다양한 기능을 쉽게 접근할 수 있는 유저 인터페이스를 갖고 있어야 한다.

(2) 기기특성

- Front panel controls	: 7”, capacitive touch surface

- Display

LCD	: Innolux LCD

Luminance	: 400 nits(400 lumen/candela per
square meter)

Resolution	: 800 x 480

- Power requirements	: +12V DC

- Power source

PoE(Power over Ethernet)	: IEEE 802.3af class 3 device via
LAN A

Optional external source(not included)	: 12V DC @ 1A(12W)

Barrel connector	: Negative contact – 5mm OD

Positive contact – 2.5mm ID

- Rear panel connectors

RJ45(x2)	: LAN A(PoE) and LAN B ports

(10/100/1000Mbps)

USB micro AB type	: USB OTG 2.0(for future use)

Barrel connector

Power inlet	: Accommodates +12 VDC power
supply

Reset button	: Recessed button
– Use a paper clip or similar

tool to reset the unit.

- Dimensions(HWD)	: 5.6” x 7.8” x 1.5”

(143mm x 198mm x 38mm)

Weight(net)	: TBD

** TSC-7w 는 동등 이상품 이어야 한다.