NETWORK VIDEO ENDPOINT

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 비디오 엔드포인트로 네트워크를 베이스로 멀티 스트리밍이 가능한 스프트웨어 구성을 갖고 있어야 하고 HDMI 인코더 및 디코더 비디오 송신이 가능한 기기여야 한다.

(2) 기기특성

[Video I/O]

- HDMI 2.0 inputs	: 3x HDMI capable of receiving

source input video

HDMI 2.0 outputs	: 2x HDMI capable of scaling and

outputting video formats up to

4K60 4:4:4

- Scaler	: Each HDMI output features a

robust, polymorphic 4K60 4:4:4

scaler that can accommodate

the most challenging resolution and

frame rate conversions.

[Audio I/O]

- HDMI inputs	: 8-channel PCM audio,

Q-SYS routable

HDMI outputs	: 8-channel PCM audio,

Q-SYS routable

- Analog audio input	: 3.5mm unbalanced stereo

mic/line input Q-SYS routable

Signal-to-noise	: 80 dB

THD+N	: 0.009% @ 0dB

Input frequency response	: 20Hz to 20kHz +0.05%/-0.5%

Input Impedance(unbalanced)	: 5kΩ nominal

Analog to digital converters	: 24 bit, 48 kHz

- Analog audio output	: 3.5mm unbalanced stereo

line output Q-SYS routable

Signal-to-noise	: 90dB

THD+N	: 0.0167% @ 0dB

Output frequency response	: 20Hz to 20kHz +0.2%/-0.5%

[General]

Dimensions	: 8.66in x 11.28in x 1.72in

(220mm x 286.6mm x 43.6mm)

- Weight	: 4.0lb(1.81kg)

[Environmental]

- Ambient operating temperature range	: 0~50°C

- Humidity	: 5 to 85% non-condensing

Storage temperature	: -20 to 70°C

[Other connectors]

RS-232	: Three-pin euroblock terminal

connector for extension of

Q-SYS control to third-party

devices, user configurable

GPIO	: Euroblock terminal connector for

extension of

Q-SYS Control to third-party

devices, user configurable

LAN A	: Gigabit LAN connection for interface

with Q-LAN;

PoE++ 802.3bt type 4 for power

LAN B	: No functionality at initial release

Power over ethernet specification/wattage	: Conforms to IEEE 802.3bt type 4

Physical power supply info	: 48V DC nominal, 1.5A on

2-pin euro connector

** NV-32-H 또는 동등 이상품 이어야 한다.