POWERED LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 10인치 파워드 라우드 스피커로 10인치 저음 드라이버와 1.4인치 네오디뮴 자석 고음 드라이버를 가지고 있어야 하고 최대 2,000W(1,300W LF + 700W HF)의 출력을 재생할 수 있어야 하며 90˚x60˚(HxV)의 지향각을 제공하는 기기여야 한다.

(2) 기기특성

[System details]

- Power output	: 2,000W peak(1,300 LF + 700 HF)

1,000W continuous RMS

(650 LF + 350 HF)

- LF driver	: 10-inch(254mm) LF driver,

2.5-inch(65mm) high-temperature

voice coil

- HF driver	: 1.4-inch(35mm) neodymium

magnet HF driver with precision

waveguide

- Crossover	: 2.5kHz

- Maximum SPL	: 129dB peak,

126dB continuous(dB SPL @ 1m)

- Frequency response	: 54Hz ~ 20kHz(+/-3dB)

- Frequency range	: 48Hz ~ 22kHz(-10dB)

- Horn coverage	: 90°H x 60°V nominal

Equalization	: Contour switch low and high

frequency +3dB boost

- Connectors	: (2) XLR/TRS 1/4”(6.35mm)

combo inputs, (1) XLR link output,

(1) IEC power cable input

- Controls	: (2) Volume, power on/off switch,

contour switch, ground-lift switch

- Indicators	: 2 x power LED(front and rear),

clip limiter LED

- Protection	: Electronic clip, thermal and

transducer overdrive protection

- Power connection	: IEC with mains fuse

- AC voltage input	: 100,110 ~ 120,220 ~ 240V,

50/60Hz

[Enclosure details]

- Enclosure	: Trapezoidal, injection-molded,

polypropylene enclosure,

with perforated steel grille

- Mounting/installation	: 36mm standard pole mount,

wall or celling mount using

TSB810 bracket, flown application

with integral M10 suspension

points, wedge monitor

- Dimensions(HxWxD)	: 20.6” x 12.6” x 11.8”/

524mm x 320mm x 300mm

- Weight(net)	: 26.1lbs./11.9kg.

- Design origin	: Designed and tuned in the USA

- Accessories	: TSB810 bracket, TS210 cover

** TS310 또는 동등 이상품 이어야 한다.