POWERED SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 파워드 서브우퍼 스피커로 12인치 저음 드라이버를 가지고 있어야 하고 최대 2,000W의 출력을 재생할 수 있어야 하며 Class D 앰프를 보유한 기기여야 한다.

(2) 기기특성

[System details]

- Power output	: 2,000W peak, 1,000W continuous

- Amplifier	: High-efficiency Class D amplifier

- Transducer	: 12”(305mm) woofer,

3”(76mm) voice coil

- Frequency response	: 44Hz ~ 95kHz(-3dB)

- Frequency range	: 38Hz ~ 110kHz(-10dB)

Macimum SPL	: 129dB(@ 1m)

126dB continuous(dB SPL @ 1m)

- Connectors	: (2) XLR/TRS 1/4”(6.35mm) inputs,

(1) XLR output,

(1) IEC power cable input

Input level	: Line +4 dBu(nominal)

- External controls	: Volume control, output mode

switch, polarity-reverse switch,

extended low-frequency switch,

power switch

- Indicators	: Signal/clip limiter LED,

polarity-reverse LED,

extended low-frequency LED,

power switch LED

- Electronic protection	: Electronic clip, thermal and

transducer overdrive protection

- Power connection	: IEC with mains fuse

- AC voltage input	: 100,110 ~ 120,220 ~ 240V,

50/60Hz

Consumption	: 1,000W

fuse: T10AL AC250V(100 ~ 120V)

or T5AL AC250V(220 ~ 240V)

[Enclosure details]

- Enclosure	: Internally braced MDF cabinet;

36mm mounting pole socket on

top panel

- Dimensions(HxWxD)	: 17.9” x 18.1” x 19.9”/

456mm x 459mm x 505mm

- Weight(net)	: 55.12lbs./25kg.

- Design origin	: Designed and tuned in the USA

- Accessories	: TS312S cover

** TS312S 또는 동등 이상품 이어야 한다.