POWERED LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 파워드 라우드 스피커로 8인치 저음 드라이버와 1인치 티타늄 고음 압축 드라이버를 가지고 있어야 하고 최대 300W(200W LF + 100W HF)의 출력을 재생할 수 있어야 하며 90˚x60˚(HxV)의 지향각을 제공하는 기기여야 한다.

(2) 기기특성

[System details]

- Power output	: 300W peak(200W LF + 100W HF),

150W continuous(100W LF + 50W

HF) Class D power

- LF driver	: 8-inch(203mm) LF driver,

1.5-inch(38.1mm) voice coil

- HF driver	: 1-inch(25.4mm) titanium diaphragm

HF compression driver

- Crossover	: 2.5kHz

- Maximum	: 113dB at 1m

- Frequency response(-3dB)	: 75Hz ~ 20kHz

- Horn coverage	: 90°H x 60°V nominal

- Connectors	: (1) XLR balanced input,

(1) XLR link output,

(1) IEC power cable input

- Controls	: (1) Volume, power on/off switch

- Indicators	: (2) Power LED(front and rear),

clip limiter LED

- Protection	: Overload analog limiter/

compressor, thermal protection

- Power supply	: 100V ~ 240V ~ 50/60Hz

- AC voltage input	: 100,110 ~ 120,220 ~ 240V,

50/60Hz

- Fuse	: 100 ~ 120V T1.6AL AC250V,

220 ~ 240V T800mAL AC250V

- Power consumption	: 150W

[Enclosure details]

- Enclosure construction	: Injection-molded polypropylene

enclosure, multi-angle for main or

monitor applications, metal grille,

rubber feet, 1 handle on top

- Mounting/Installation	: Standard speaker pole socket,

wedge monitor

- Dimensions(HxWxD)	: 16.6" x 10.7 x 9.9"/

422mm x 272mm x 252mm

- Weight(net)	: 13.9lbs./6.3kg.

** TX208 또는 동등 이상품 이어야 한다.