POWERED LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 15인치 파워드 라우드 스피커로 15인치 저음 드라이버와 1인치 네오디뮴 고음 압축 드라이버를 가지고 있어야 하고 최대 600W(400W LF + 200W HF)의 출력을 재생할 수 있어야 하며 90˚x60˚(HxV)의 지향각을 제공하는 기기여야 한다.

(2) 기기특성

[System details]

- Power output	: 600W peak(400W LF + 200W HF),

300W continuous(200W LF + 100W

HF) Class D power

- LF driver	: 15-inch(381mm) LF driver,

2-inch(50.8mm) voice coil

- HF driver	: 1-inch(25.4mm) neodymium HF

compression driver

- Crossover	: 2.2kHz

- Maximum	: 119dB at 1m

- Frequency response(-3dB)	: 65Hz ~ 20kHz

- Horn coverage	: 90°H x 60°V nominal

Equalization	: Contour switch low and high

frequency +3dB boost

- Connectors	: (1) XLR/TRS 1/4”(6.35mm) combo

input, (1) XLR link output,

(1) IEC power cable input

- Controls	: (1) Volume, power on/off switch,

contour switch, ground-lift switch

- Indicators	: (2) Power LED(front and rear),

clip limiter LED

- Protection	: Overload analog limiter/

compressor, thermal protection

- Power supply	: 100V ~ 240V ~ 50/60Hz

- AC voltage input	: 100,110 ~ 120,220 ~ 240V,

50/60Hz

- Fuse	: 100 ~ 120V T4AL AC250V,

220 ~ 240V T2AL AC250V

- Power consumption	: 260W

[Enclosure details]

- Enclosure construction	: Injection-molded polypropylene

enclosure, multi-angle for main or

monitor applications, metal grille,

rubber feet, 2 handles(both sides)

- Mounting/Installation	: Standard speaker pole socket,

wedge monitor

- Dimensions(HxWxD)	: 24.7" x 15.2" x 14.6"/

627mm x 386mm x 371mm

- Weight(net)	: 32.4lbs./14.7kg.

** TX215 또는 동등 이상품 이어야 한다.