COMPACT PA SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 소형 고성능 PA 스피커로 6인치 저음 드라이버와 1인치의 네오디뮴 고음 압축 드라이버를 사용하면서 2-way 형태여야 하고 최대 200W(130W LF + 70W HF)의 출력을 제공해야 하며 열 또는 과부하로부터 장비를 보호할 수 있는 기능이 내장되어있는 기기여야 한다.

(2) 기기특성

[System details]

- System type	: 2‐way biamplified compact

PA system for the active performer
- High frequency	: 25mm(1inch) voice coil

neodymium compression driver
- Low frequency	: (3) 6 1/2”(165mm) woofers with

1” voice coil

- Frequency range	: 65 to 20kHz

- Crossover	: 1.8kHz, electronic

- Power amplifier	: Bi-amplified, 200watt peak

(130W LF + 70W HF)
- Maximum SPL	: 117dB-SPL @ 1m(continuous),

120dB-SPL @ 1m(peak)

- Electronic protection	: Thermal/overload

Protection indication	: Signal/limit red LED

Inputs	: 3 channels(line/mic 1, line/mic

2, aux)

Input connectors	: (2) 1/4” XLR female combo

connectors,  (1) stereo RCA,

(1) 1/8” stereo

Output connectors	: (1) XLR male mix output

Equalization	: 2-band LF and HF

Bluetooth	: A2DP streaming audio, with full

stereo link when using

two troupers

- Power controls	: on/off power switch, IEC line cord

AC input, Power indicator LED

[Enclosure details]

Enclosure type	: Trapeziodal MDF enclosure with

black vinyl wrap and protective

steel corners

Handle	: Rear mounted,

ergonomically designed

- Stand mount socket	: (1) female 36mm pole socket

- Dimensions	: 8.4 x 29.2 x 10.1in/

21.3 x 74.17 x 25.65cm

Weight	: 23lbs/10.43kg

** TROUPER 또는 동등 이상품 이어야 한다.