BLUETOOTH PA SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 블루투스 PA 스피커로 6.5인치 저음 드라이버와 2인치 고음 드라이버를 사용하면서 2-way 형태여야 하고 최대 50W의 출력을 제공해야 하며 내장 배터리 형태로 충전이 가능하여 최대 50시간 연속으로 사용 할 수 있는 기기여야 한다.

(2) 기기특성

[System details]

- Power output	: 50watts peak

(25watts continuous power)
- LF driver	: 6.5-inch(165.1mm) woofer
- HF Drive	: 2-inch(50.8mm) tweeter

- Frequency response	: 90Hz ~ 20kHz

- Connectors	: (2) line/mic channels with

XLR-1/4-inch(6.35mm)

TRS combination input,

(1) 1/8-inch(3.5mm)

TRS/stereo aux input,

(1) 1/4-inch(6.35mm) line-out,

(1) IEC AC power connection with

mains fuse

- Charge port	: (1) USB +5V, 1A
- Controls	: (2) Volume controls for

line/mic channels,

(2) line/mic selectors,

(1) volume control for

bluetooth® and aux channels,

master volume,

bluetooth® pairing button,

power on/off switch

- Indicators	: Power on, battery level,

bluetooth® pairing status.

Bluetooth®	: Profile-A2DP, AVRCP,

range-up to 100feet/30.5meters

Bluetooth® connection	: Manual pairing or NFC

Battery type	: 12V, 5.0Ah SLA

Battery life	: Built in rechargeable battery

delivers up to 50hours of

continuous use

Power	: 100 ~ 240V AC, 50/60Hz

AC voltage input/fuse	: 100, 110 ~ 120, 220 ~ 240V/

T630mAL AC250V

[Enclosure details]

- Dimensions(HxWxD)	: 13.8”x16.2”x9.4”/

351mm x 412mm x 242mm

Weight	: 16.5lbs./7.7kg.

** UBER PA 또는 동등 이상품 이어야 한다.