ACTIVE STAGE MONITOR SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 액티브 무대 모니터 스피커로 12인치 저음 드라이버와 1인치 네오디뮴 고음 드라이버를 가지고 있어야 하고 최대 800W(670W LF + 130W HF)의 출력을 재생할 수 있어야 하며 70˚x70˚(HxV)의 지향각을 제공하는 기기여야 한다.

(2) 기기특성

[System details]

- Power system	: Continuous : 400W(335W LF +

65W HF),

peak : 800W(670W LF + 130W HF)

- Maximum SPL @ 1m	: 118dB continuous/121dB peak

- Coverage	: 70°H x 70°V spherical horn

- Transducer low	: 12” coax/2” voice coil

- Transducer high	: 1” neodymium driver/1” voice coil

- Protection	: Low ~ high analog limiter

- Electronic protections	: Modeller with 16 preset/

line volume/clipping LED indicator/

ground switch

- Input level	: Line +4 dB

- Input impedance	: 30kΩ balanced/15kΩ unbalanced

Input connector	: Combo Jack with XLR/TRS

- External control	: Volume control/power on with

green LED/clip limiter with

red LED/ground lift

- Power supply	: AC ~ 220/240V or AC – 110/120

volt, with switching power mode.

[Enclosure details]

- Cabinet	: Trapezoidal shape/multi-layer

plywood/handle/black paint

finishing

- Dimensions(HxWxD)	: 313mm x 393mm x 513mm

- Weight(net)	: 26.12Ibs./11.85kg

** SXM112A 또는 동등 이상품 이어야 한다.