NETWORK/BLUETOOTH AUDIO INTERFACE

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 유/무선 형태의 Dante/AES67 네트워크, 아날로그, 블루투스로 연결하여 오디오 신호를 주고받을 수 있어야 하고 하나의 버튼으로 간편한 페어링이 가능한 동시에 다중 프로세서에 페어링 연결을 지원해야 하며 아이패드, 태블릿 또는 휴대용 스마트폰과 연결 및 호환 가능한 기기여야 한다.

(2) 기기특성

System details

- Bluetooth profile	: A2DP - stereo audio is streamed

from a bluetoothdevice and -

onto the dantenetwork.

HFP(Hands Free Profile) -

duplex pairing to a cell phone for

call bridging

- Bluetooth range	: 10m(30ft) minimum. typical range

is 15 ~ 23m(50 ~ 75ft)

- RCA and 3.5 mm input	: RF filtered line level, input source

software selectable

- Maximum input levels(3.5mm / RCA)	: +12dBu

- Output volume range	: 0dB to -60dB in 1dB steps,

software selectable

- Output noise	: < -90dBu @ 0dB gain

- 3.5mm output	: RF filtered line level

- Maximum output level(3.5mm)	: +12dBu

- System THD	: < 0.02% at any gain, input signal

3dB below maximum

(wired I/O only)

- Certifications	: FCC 47CFR parts 15B and

18(Class A), EN 55011, ICES-003,

CE(EN55022 Class A and EN55024

Class A)

- Product dimensions(WHD)	: 3.54 x4.2x1.88in

(89.91 x 106.68 x 47.752mm)

- Shipping dimensions(WHD)	: 6 x 6 x 43.54 x 4.2 x 2in

(152.4 x 152.4 x 101.6mm)

- Shipping weight	: 1.0lb(0.4536kg)

- Operating temperature	: 0°C – 40°C

** unD6IO-BT 또는 동등 이상품 이어야 한다.