BLUETOOTH AUDIO INTERFACE

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 무선 형태의 블루투스로 연결하여 오디오 신호를 주고받을 수 있어야 하고 하나의 버튼으로 간편한 페어링이 가능한 동시에 다중 프로세서에 페어링 연결을 지원해야 하며 아이패드, 태블릿 또는 휴대용 스마트폰과 연결 및 호환 가능한 기기여야 한다.

(2) 기기특성

System details

- Bluetooth profile	: A2DP - stereo audio is streamed

from a Bluetooth device to the

unBT2A and output as analog

(via the unBT2A EXP interface)

- Bluetooth range	: 30 ~ 70ft typical

- Depluggableoutput type	: Balanced 3-pin line level,

-10dBV/+4dBu nominal

output levels(software switchable)

on the unBT2A EXP. mono/stereo

functionality is also software

switchable

- Dynamic range	: > 85dB

- Maximum output level(balanced depluggable)	: +20dBu in +4dBu setting, +6dBu in

-10dBV setting

- System THD	: Less than 0.1%

- RS-232	: Full RS-232 control

(standard RS-232 levels) of pairing

and other user interface features.

3-pin depluggableconnector on the

unBT2A EXP

- USB	: Mini B type connector

- Certifications	: FCC 47CFR Parts 15B and 18

(Class A), EN 55011, ICES-003,

CE(EN55022 Class A and EN55024

Class A

- Dimensions(WHD)	: unBT2A - 1.69 x 4.2 x 1.25in

(42.93 x 106.68 x 31.75mm)

unBT2A EXP -5.56 x 1.13 x 1.75in

(141.22 x 28.7 x 44.45mm)

- Operating temperature	: 0°C – 40°C

** unBT2A 또는 동등 이상품 이어야 한다.