NETWORK AUDIO ENDPOINT

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 AES67 네트워크, 아날로그로 연결하여 오디오 신호를 주고 받을 수 있어야 하고 PoE 및 48V 팬텀 전원 공급이 가능하고 소프트웨어를 통한 입출력, 팬텀 전원, 프리앰프 등 제어가 가능하며 테이블 및 랙에 장착시킬 수 있는 기기여야 한다.

(2) 기기특성

System details

Audio inputs(mic/line)

- Connector type	: 3.81mm euro-block, 3position

(16 ~ 28AWG)

- Gain	: -8dB to +34dB gain,

1dB increments

- Input impedance	: > 2kΩ at any gain

- Maximum input levels	: -8dB gain, max input =

+16.5dBu(+24dBu w/pad)

- Phantom power	: +48V, software selectable

per channel

- THD+N	: < 0.05% @ 1kHz, -3dBFS input.

20 ~ 20kHz

- Frequency response	: 20 ~ 20kHz, +/-1dB(line),

50 ~ 20kHz +/-1dB(mic)

- EIN	: -125dBu

Audio outputs(mic/line)

- Connector type	: 3.81mm euro-block, 3position

(16 ~ 28AWG)

- Maximum output levels	: +24dBu(-15.5dBU w/pad)

- THD+N	: < 0.05% @ 1kHz, -3dBFS output.

20 ~ 20kHz

- Frequency response	: 20 ~ 20 kHz, +/-1dB(line),

50 ~ 20kHz +/-1dB(mic)

- Dynamic range	: 100dB

Network

- Physical layer	: Ethernet

- Connector(s)	: Dual RJ-45

- Cable quality	: CAT-5e or better, UTP

- Transmission speed	: 1Gbps

Power

- PoE power	: 802.3.af/at Class 0

- Power consumption	: < 10W(with phantom power

enabled and powered by 24V DC),

< 12W(on PoE)

- Power options	: PoE, +24V DC(PoE and external

DC can be used for redundancy)

General

- Dimensions(WHD)	: 7.4 x 1.6 x 8in

(188 x 40.6 x 203mm)

- Weight	: 2.1lbs(0.95kg)

- Mounting options	: Rack-mountable, 1RU 1/3-rack

width surface-mountable

*all mounting hardware offered as

accessories

- Regulatory compliance	: FCC part 15, subpart B,

Class A EMC CE

(EN55032 EMC / EN55035 ESD)

WEEE RoHS REACH

Environmental

- Operating temperature	: 0 to 40°C

** Axon A8Mio 또는 동등 이상품 이어야 한다.