EMBBEDDER/DE-EMBEDDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Dante/AES67 네트워크, 아날로그로 연결하여 오디오 신호를 HDMI로 비디오를 연결하여 비디오 신호를 서로 합성하여 HDMI로 출력이 가능하고 또는 HDMI로 연결하여 오디오 신호와 비디오 신호를 분리하여 출력할 수 있으며 비디오 신호는 최대 4:4:4/4K/60Hz의 해상도를 지원하는 기기여야 한다.

(2) 기기특성

System details

Analog audio inputs

- Input type	: Balanced 3-pin line level

- Input sensitivity	: –10dBV(consumer) or

+4dBu(professional),

software-selectable

- Input impedance	: 10kΩ

- Maximum input levels	: +20dBu(+/- 0.5dB) @

+4dBu input sensitivity,

+10dBV (+/- 0.5dB) @

-10dBV input sensitivity

- THD+N	: < 0.005%

- Dynamic range	: > 105dB

Analog audio output

- Output type	: Balanced 3-pin line level

- Output impedance	: –10dBV(consumer) or +4dBu(pro)

software selectable

- Maximum output level	: 10kΩ

- THD+N	: +20dBu(+/- 0.5dB) @

+4dBu input sensitivity,

+10dBV(+/- 0.5dB) @

-10dBV input sensitivity

S/PDIF audio inputs

- Supported formats	: S/PDIF(IEC-60598) 2ch PCM, 24bit

- Supported sample rates	: 44.1kHz, 48kHz, 88.2kHz,

96kHz, 192kHz

- THD+N	: < 0.005%

S/PDIF audio output(mirrors HDMI input audio)

- Supported formats	: S/PDIF(IEC-60598) 2ch PCM,

24bit compressed multi-channel in

pass through mode

- Supported sample rates	: 44.1kHz, 48kHz, 88.2kHz,

96kHz, 192kHz

- THD+N	: < 0.005%

HDMI audio inputs/outputs

- Supported formats	: 2-CH PCM, 24bit

- Supported sample rates	: 44.1kHz, 48kHz, 88.2kHz,

96kHz, 192kHz

- THD+N	: < 0.005%

Video specifications

- HDCP	: S/PDIF(IEC-60598) 2-CH PCM,

24bit compressed multi-channel in

pass through mode

- HDMI	: 44.1kHz, 48kHz, 88.2kHz,

96kHz, 192kHz

- Supported video formats	: Resolution/frame rate(Hz) -

4096 x 2160p/23.98, 24, 25, 29.97,	30, 50, 59.97, 60

3840 x 2160(UHD)/23.98, 24, 25,

29.97, 30, 50, 59.97, 60

2048 x 1080p, 1080p/23.98, 24,

25, 29.97, 30, 50, 59.94, 60

1080i, 720p, 576p, 576i, 480p/480i

50, 50.94, 60

3D support

- Color space	: YUV, RGB

- Chroma subsampling	: 4:4:4, 4:2:2, 4:2:0

- Max color depth	: 48bit

- EDID	: SW configurable

- Hot plug detect	: SW configurable

- Bandwidth	: 18Gbps(600MHz)

- Connectors	: HDMI type A

Dante network

- Physical layer	: Ethernet

- Connector	: Single RJ-45

- Cable quality	: CAT-5e or higher

- Transmission speed	: 100Mbps

- Supported sample rates	: 48kHz

- Minimum Dante network latency	: 1ms

Power requirements

- PoE	: 802.3af PoE PD compliant

- Power consumption	: < 7.6W max

General

- Dimensions (WHD)	: 9.2 x 1 x 4in

(233.7 x 25.4 x 101.6mm)

- Weight	: 1.3lb(0.6kg)

- Product compliance	: CC CFR 47 parts 15B Class A,

EN55011, ICES-003, CE

(EN55022 / EN55024), RoHS,

REACH

** unHX2D 또는 동등 이상품 이어야 한다.