NETWORK AUDIO INTERFACE

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Dante/AES67 네트워크, 아날로그를 연결하여 오디오 신호를 주고받을 수 있고 모니터링을 위한 헤드폰 및 라우드 스피커를 내장되어 있으며 기본 32채널. 확장하여 최대 128채널의 신호를 모니터링이 가능한 기기여야 한다.

(2) 기기특성

System details

Audio inputs

- Maximum input level	: +24dBu

- Input impedance	: 10kΩ

- Input type	: 3-pin XLR-F

- Dynamic range	: > 105dB

- THD+N	: < 0.02% @ -3sBFS

- Frequency response	: 20Hz to 20kHz, +/- 0.5dB

Audio outputs

- Maximum output level	: +24dBu

- Output impedance	: 200Ω

- Input type	: 3-pin XLR-M

- Dynamic range	: > 110dB

- THD+N	: < 0.02% @ -3dBFS

- Frequency response	: 20Hz to 20kHz, +/- 0.5dB

Headphone output

- Connector	: 1/4 in TRS jack

- Controls	: Mute/volume encoder

- Load	: 32Ωminimum

Audio networking

- Protocol support	: Dante with AES67 support

- Channel count	: 32 Dante RX, 2 Dante TX

- Modes	: Switched or redundant mode

- Latency	: 0.250ms minimum

- Ports	: 2 - Gb copper on RJ-45,

2 - Gb SFP

Digital I/O

- AES-3	: AES-3 digital output on 3-pin

XLR-M

- Word clock	: Sync I/O on BNC with switchable

75ohm termination on input

Environmental

- Power	: 110V-220V AC input, with optional

external 24V DC redundant supply

- Power consumption	: < 20W

General

- Dimensions(WHD)	: 1 RU form factor

19 x 1.75 x 12.5in

(482.6 x 44.5 x 317.5mm)

- Weight	: 6lb(2.72kg)

- Operating temperature	: 0 to 40°C

- Regulatory compliance	: FCC 47CFR parts 15B and 18

(Class A), EN 55011, ICES-003,

CE(EN55032 Class A and EN55024

Class A)

** Synapse DM1 또는 동등 이상품 이어야 한다.