NETWORK PAGING STATION

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Dante/AES67 네트워크, 아날로그로 연결하여 최대 4개의 zone을 설정하여 원하는 zone의 버튼을 선택했을 때 해당 zone으로 출력할 수 있고 PoE 및 48V 팬텀 전원 공급이 가능하며 소프트웨어를 통해 입출력, 팬텀 전원 등 제어가 가능한 기기여야 한다.

(2) 기기특성

System details

- Zone buttons	: Four, white backlit, each with an

associated bicolor status LED.

LED state is fully controlled over

the network, and button state can

be monitored over the network.

- Ready and busy	: Bi-color ready and busy system

status LEDs. LED state is full

controlled over the network

- Microphone/PTT input	: RJ-45 and side-mounted

6-pin depluggable. PTT input is

dry contact, closed is active

- Microphone gain	: +25dB(with automatic

phantom power) and +35dB

- Power consumption	: < 5W max, 802.3af PoE

PD compliant

- Certifications	: FCC 47CFR parts 15B and

18(Class A), EN 55011, ICES-003,

CE(EN55022 Class A and EN55024

Class A)

- Dimensions(WHD)	: 4.57 x 4.49 x 1.5 in

(106.07 x 114.04 x 48.9mm)

- Operating temperature	: 0°C – 40°C

** Zip4 또는 동등 이상품 이어야 한다.