AUDIO EXPENSION MODULE

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Dante 네트워크, 아날로그, USB로 연결하여 최대 64개의 채널 중 선택하여 내부 스피커로 모니터링 할 수 있고 USB 연결을 이용하여 핸드프리 형식으로 USB 웹 회의 오디오 인터페이스로도 사용할 수 있으며 PoE 전원 공급이 가능한 기기여야 한다.

(2) 기기특성

System details

Audio inputs

- Input types : Internal electret microphone, External electret headset microphone connectivity with internal bias(3.5mm T-S), Line input: 3.5mm TRS

- Input impedance : Line input: 10kΩ

- Maximum input levels : Line input: +12dBu

- Mic bias voltage : 1.65V

Audio input performance

- THD+N ; Line input: < 0.02% @ 1kHz

- Frequency response : Line input: 20Hz–20kHz, +/-1dB

Audio outputs

- Speaker type : Internal 1in driver

- Attenuation range : Software-controlled volume, 1 to 10(max), 6dB per step

- Headphone output : Stereo 3.5mm TRS

- Maximum output levels : Loudspeaker: 1W @ max volume, Headphone: 1Vrms into 32Ω(minimum load)

Audio output performance

- THD+N : < 0.01% @ 1kHz, input signal 3dB below maximum

- Frequency response : Headphone: 20Hz–20kHz +/-1dB

Dante network

- Physical level : Ethernet

- Connector(s)  : Dual RJ-45

- Cable quality : CAT-5e or greater

- Transmission speed ; 1000Mbps

- Supported sample rates : 48kHz

- Minimum Dante network latency : 1ms

Power requirements

- PoE : 802.3af PoE PD compliant

- External power : 24V DC, center positive barrel jack, 6.0mm OD/2.0mm ID

- Power consumption : < 6W max

General

- Product compliance : FCC CFR 47 parts 15B, ICES-003, CE(EN55022), RoHS, REACH

- Dimensions(WHD) : 6.45 x 2.6 x 6.23in(163.83 x 66.04 x 158.24mm)

- Weight : 1.13lb(0.51Kg)

** unDNEMO 또는 동등 이상품 이어야 한다.