COMPACT POWERED SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 2Way 스피커로 경량의 1,000W 클래스 D 앰프를 내장한 스피커이어야 한다. DMT™ (Directivity Matched Transition)의 기술이 적용되어 모든 청음 영역에서 LF와 HF의 커버리지를 매칭시켜 상쇄되거나 지나치게 부스트 되는 주파수 영역을 제거할 수 있어야 하고 Intrinsic Correction™ 기술이 적용되어 평탄한 음압재생, 주파수 손상 없이 저음역 제어, 내장된 앰프를 클립핑 신호로부터 보호할 수 있어야 하는 기기이어야 한다.

(2) 기기특성

- Configuration	: Two-way active loudspeaker

- LF transducer	: 12in(305mm), cone

- HF transducer	: 1.4in(35.6mm) compression driver

- Frequency response(-6dB)	: 49Hz~20kHz

- Frequency range(-10dB)	: 47Hz~20kHz

- Nominal coverage Angle	: 75° axisymetric

- Maximum rated SPL	: 126dB

- Amplifier	: Class D
Peak; 800W(LF), 200W(HF)

- Controls	: Power

2 x Gain

Mic boost push switch

6-way contour selection switch

- Indicators	: Power LED

2 x input signal LED

input B MIC selected LED

Limiter active LED

- Connectors	: 2 x locking XLR/F ¼” combo
(Line input and mic/line input)
1 x 3.5mm TRS(Stereo input)

1 x XLR/M(Mix Output)
1 x IEC power connector

- AC power input	: Universal power supply
100~240 VAC, 50~60 Hz

- AC power consumption(1/8th Power)	: 100 VAC, 0.75A~240VAC, 0.31A

- Enclosure material	: Polypropylene

- Attachment points	: 2 x M8 threaded insert
(for yoke mount attachment only)

- Color	: Black

- Grille	: 18 Gauge powder coated steel

- Dimensions(H x W x D)	: 20.3 x 13.8 x 12.7 in
516 x 350 x 323 mm

- Net weight	: 30.3lbs(13.7kg)

- Shipping weight	: 36.3lbs(16.5kg)

** CP-12 또는 동등 이상품 이어야 한다.