MULTI-CHANNEL AMPLIFIERS

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 4채널 앰프로서 4Ω, 8Ω, 70V, 100V 모드를 지원하며 모든 채널에 200W를 지원하며 28분 동안 사용하지 않을 시 대기 모드로 전환되는 기능을 지원하여야 한다.

(2) 기기특성

- Channels	: 8

[Power(all channels driven)]

- 4Ω	: 200W

- 8Ω	: 200W

- 70V	: 200W

- 100V	: 200W

- FlexAmp technology	: Allows each pair of amplifier
channels to deliver up to 400W
total power, in any ratio

- Typical distortion(4-8 Ω)	: <0.01%

- Maximum distortion(4-8 Ω)	: <1%

- Damping factor	: 100

- Output circuitry	: Class D

- Protection	: Short circuit, open circuit,
over current, thermal,
RF protection, DC fault,
inrush limiting

- Gain at 8Ω	: 30 dB

- Input impedance	: >10k, balanced or unbalanced

- Input sensitivity	: 1.23V(+4dBu)

- Maximum input level	: 12.3V(+24dBu)

- Frequency response at 8Ω	: 20Hz~20kHz +/-0.5dB

- Signal to noise	: >103dB

- User-configurable operating modes(per channel)
: DIP switch selectable,
low impedance 4Ω or 8Ω,
high impedance direct drive 70V or
100V

- Highpass filter	: 80Hz DIP switch engaged per
channel

[Cooling]

- Type	: Forced air cooling, thermally
regulated fan speed,
side/rear-to-front airflow

- Operating temperature range	: Maximum; -10°~50° C,
recommended; 0°~35° C,
performance may be reduced
above 40°C

[Connectors]

- Input connectors	: Four 3.5mm Euro, 3-pin(green)

- Remote connectors	: One 3.5mm Euro, 5-pin(black)

- Output connectors	: Two 5.0mm Euro, 4-pin(green)

- Front panel indicators	: Power, signal(per channel),
limit/mute/protect (per channel)

- Rear panel indicators	: Bi-Color LED signal/limit/mute/
protect

- Remote I/O	: Remote standby, amplifier status
enunciation on 3.5mm connectors

- AC Power input	: Universal power supply with PFC,
100~240 VAC, 50~60 Hz

- Agency approvals	:  UL, CE, RoHS/WEEE compliant,
FCC Class B(conducted and
radiated emissions)

- Dimensions(HWD) inches	: 1.75in x 19in x 14.8in

- Dimensions(HWD) mm	: 44mm x 483mm x 377mm

- Net weight	: 9.3lb(4.2kg)

- Shipping weight	: 13.9lb(6.3kg)

** MP-A40V 또는 동등 이상품 이어야 한다.