POWERED LINE ARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2웨이 라인어레이 스피커로서 설치에 적합하게 설계돼 상대적으로 넓은 범위를 지닌 장소에서도 성능이 떨어지지 않도록 수직 배열할 수 있어야 한다. 500W x 500W의 파워앰프를 내장한 기기로 90°의 수평 18°의 수직 커버리지를 가지며 Ar-Q™의 기술이 적용되어 신속하게 주파수 최적화를 위해 다이얼 클릭으로 스피커 배열이 가능하고 12인치의 저역대 유닛과 1.75인치의 컴프레션 드라이버를 장착하고 있는 기기이어야 한다.

(2) 기기특성

- Configuration	: Multipurpose 2-way

- Transducers
Low-Frequency	: 12" cone transducer
High-Frequency	: 1.75" diaphragm compression driver

- Frequency Response(-6dB)	: 49Hz~18kHz

- Frequency Range(-10dB)	: 44Hz~20kHz

- Nominal Coverage(-6dB)	: 90 x 18 degree

- Maximum SPL(1 meter)	: 131 dB peak

- Amplifiers
Power Output	: 500W x 500W power module

- Input Impedance(Ω)	: XLR; 40k balanced/20k unbalanced

- Controls	: Power·Attenuation·LF Setting
(External Sub/Normal/DEEP™)·
Array Size(1-5)·Front LED(Pwr/
Limit/Off)

- Indicators	: Limit·Standby·Power·Signal

- Connectors	: Balanced female XLR line level
input·Balanced male XLR full range
line level out·Remote attenuation
control·Locking powerCON® power
connector AC out

- Cooling	: On demand, 50mm variable speed
fan

- Amplifier Protection	: Thermal limiting·Output
overcurrent·Overtemperature
muting·GuardRail™

- Transducer Protection	: Thermal limiting·Excursion limiting

- AC Power Input	: Universal power supply
100~240 VAC, 50~60 Hz

- AC Power Consumption	: 100VAC, 2.3A·120VAC, 2.01A·
230VAC, 1.13A

- Enclosure	: Impact resistant ABS

Weight(Net)	: 55lbs(25kg)

Finish	: Black or White paint

Grille	: Black or White powder coated

18 gauge steel

- Dimensions(HWD)	: 15.0" x 23.4" x 16.6“

(381mm x 594mm x 422mm)

- Available Accessories	: KLA12 TOTE·K Series M10 KIT·

KLA AF12 Array Frame

** KLA12 또는 동등 이상품 이어야 한다.