LOUD SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6인치 2Way 스피커로 DMT(Directivity Matched Transition) 기능으로 음의 영역을 균일하게 하고 부드러운 주파수 응답을 보장하여야 한다. IEC60529 IP-54 등급으로 먼지와 얼룩 저항성 및 방수가 가능하여야 한다. 내후성을 강화하기 위해 밀폐형 입력패널 덮개와 분말 코팅된 알루미늄 그릴을 사용하여야 한다. 내장된 스피커 브라켓은 특허받은 X-MOUNT 기술로 스피커를 쉽고 빠르게 설치하며 설치 후 변형이 없어야 한다. 이 통합된 기기이어야 한다.

(2) 기기특성

- HF transducer	: 1”silk dome tweeter/1”voice-coil

horn loaded

- LF transducer	: 6.5”weather treated paper cone

woofer, 1.5”/38mm voice-coil

- Effective frequency range	: 58Hz~20kHz

- Rated noise power(voltage)	: 150watts/49V(rms)

- Broad-band sensitivity	: 89dB SPL

- Coverage angle(-6dB)	: 105°

- Directivity factor(Q)	: 5

- Directivity Index	: 7dB

- Maximum continuous SPL	: 110dB

- Maximum peak SPL	: 116dB

- Rated impedance	: 16Ω

- Recommended amplifier	: 300W

- Input connector type	: Euroblock connector with parallel

output

- Enclosure material	: Painted ABS polymer

- Grille material	: Powder coated aluminum

- Ingress protection	: IP-54

- Operating environment	: Designed for indoor and outdoor

use

- Operating Temperature Range	: -20 to 50°C/-4 to 122°F

- Net weight	: 11.6Ibs/5.26kg

- Product dimensions	: 14.4” x 8.5” x 8.5”

(365 x 215 x 215mm)

- Shipping weight	: 28.7Ibs/13.02kg(pair packed)

- Shipping dimensions	: 20” x 12” X 23”

(510 x 305 x 585 mm)

(pair packed)

** AD-S6 또는 동등 이상품 이어야 한다.